<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="13.573125" y1="21.55825" x2="9.001125" y2="21.55825" width="0" layer="20"/>
<wire x1="9.001125" y1="21.55825" x2="8.366125" y2="20.92325" width="0" layer="20" curve="90"/>
<wire x1="8.366125" y1="20.92325" x2="8.366125" y2="14.2875" width="0" layer="20"/>
<wire x1="8.366125" y1="14.2875" x2="-0.28575" y2="14.2875" width="0" layer="20"/>
<wire x1="-0.28575" y1="14.2875" x2="-0.92075" y2="13.6525" width="0" layer="20" curve="90"/>
<wire x1="-0.92075" y1="13.6525" x2="-0.92075" y2="12.065" width="0" layer="20"/>
<wire x1="-0.92075" y1="12.065" x2="-0.28575" y2="11.43" width="0" layer="20" curve="90"/>
<wire x1="-0.28575" y1="11.43" x2="8.366125" y2="11.43" width="0" layer="20"/>
<wire x1="8.366125" y1="11.43" x2="8.366125" y2="2.079625" width="0" layer="20"/>
<wire x1="8.366125" y1="2.079625" x2="9.144" y2="1.444625" width="0" layer="20" curve="90"/>
<wire x1="9.144" y1="1.444625" x2="20.712059375" y2="1.444625" width="0" layer="20"/>
<wire x1="20.712059375" y1="1.444625" x2="21.351875" y2="2.076846875" width="0" layer="20" curve="89.749333"/>
<wire x1="21.351875" y1="2.076846875" x2="21.351875" y2="20.92325" width="0" layer="20"/>
<wire x1="21.351875" y1="20.92325" x2="20.716875" y2="21.55825" width="0" layer="20" curve="90"/>
<wire x1="20.716875" y1="21.55825" x2="16.8275" y2="21.55825" width="0" layer="20"/>
<wire x1="16.8275" y1="21.55825" x2="16.8275" y2="22.5407" width="0" layer="20"/>
<wire x1="16.8275" y1="22.5407" x2="15.317575" y2="23.97125" width="0" layer="20" curve="90"/>
<wire x1="15.317575" y1="23.97125" x2="14.97135625" y2="23.97125" width="0" layer="20"/>
<wire x1="14.97135625" y1="23.97125" x2="13.573125" y2="22.33489375" width="0" layer="20" curve="90"/>
<wire x1="13.573125" y1="22.33489375" x2="13.573125" y2="21.55825" width="0" layer="20"/>
<hole x="15.1765" y="22.386925" drill="1.5875"/>
<text>+</text>
<text>sonde02</text>
<text>protofusion</text>
<text>-</text>
</plain>
<libraries>
<library name="Ava">
<packages>
<package name="QFN20+GNDPAD">
</package>
</packages>
</library>
<library name="Protofusion">
<packages>
<package name="UFQFPN28">
</package>
<package name="POGOPROG-CONN-4-ALLSMT">
</package>
<package name="TSOT23-6">
</package>
<package name="FEATHERHAB-ALPHA">
</package>
<package name="WIREPAD">
</package>
</packages>
</library>
<library name="picoAVA-R9">
<description>Generated from &lt;b&gt;picoAVA-R9.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="AVA_JTI_ANTENNA-1575AT43A40">
</package>
<package name="AVA_UBLOX_MAX-6">
<description>uBlox MAX-6</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1210">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SLAT-Connectors">
<description>SLAT Connectors</description>
<packages>
<package name="JST_ZH-V-2-1">
</package>
</packages>
</library>
<library name="SLAT-Digital">
<description>SLAT Digital</description>
<packages>
<package name="HCLGA-10L">
</package>
</packages>
</library>
<library name="Protofusion-passives">
<packages>
<package name="0402-CAP">
</package>
<package name="0402-INDUCTOR">
</package>
<package name="0603-RES">
</package>
<package name="0402-RES">
</package>
<package name="0603-CAP">
</package>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="SLAT-Transistors">
<description>SLAT Transistors</description>
<packages>
<package name="SC-75A">
</package>
</packages>
</library>
<library name="SLAT-Analog">
<description>SLAT Analog</description>
<packages>
<package name="ASDM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Ava" package="QFN20+GNDPAD" value="SI4463"/>
<element name="U2" library="picoAVA-R9" package="AVA_JTI_ANTENNA-1575AT43A40" value="AVA_JTI_ANTENNA-1575AT43A40"/>
<element name="U7" library="picoAVA-R9" package="AVA_UBLOX_MAX-6" value="AVA_UBLOX_MAX-6"/>
<element name="U6" library="Protofusion" package="UFQFPN28" value="STM32F031G6U6"/>
<element name="J1" library="Protofusion" package="POGOPROG-CONN-4-ALLSMT" value="POGOPIN-CONN-4">
<attribute name="VALUE"/>
</element>
<element name="U4" library="Protofusion" package="TSOT23-6" value="LTC3531-3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="1210" value="LQH32CN100K33L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="Protofusion" package="FEATHERHAB-ALPHA" value=""/>
<element name="D1" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND-1" library="Protofusion" package="WIREPAD" value="WIREPAD">
<attribute name="VALUE"/>
</element>
<element name="ANT" library="Protofusion" package="WIREPAD" value="WIREPAD">
<attribute name="VALUE"/>
</element>
<element name="GND-2" library="Protofusion" package="WIREPAD" value="WIREPAD">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SLAT-Connectors" package="JST_ZH-V-2-1" value="JST_ZH-V-2-1">
<attribute name="VALUE"/>
</element>
<element name="U5" library="SLAT-Digital" package="HCLGA-10L" value="LPS25H">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CM1" library="Protofusion-passives" package="0402-CAP" value="12pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CM" library="Protofusion-passives" package="0402-CAP" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CM2" library="Protofusion-passives" package="0402-CAP" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C0" library="Protofusion-passives" package="0402-CAP" value="9.1pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LM3" library="Protofusion-passives" package="0402-INDUCTOR" value="22nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LM2" library="Protofusion-passives" package="0402-INDUCTOR" value="36nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LM1" library="Protofusion-passives" package="0402-INDUCTOR" value="30nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L0" library="Protofusion-passives" package="0402-INDUCTOR" value="33nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCHOKE" library="Protofusion-passives" package="0402-INDUCTOR" value="220nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Protofusion-passives" package="0402-CAP" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Protofusion-passives" package="0402-CAP" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Protofusion-passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Protofusion-passives" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Protofusion-passives" package="0402-RES" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="Protofusion-passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="Protofusion-passives" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SLAT-Transistors" package="SC-75A" value="SSM3J36FS,LF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="Protofusion-passives" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="Protofusion-passives" package="0402-RES" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Protofusion-passives" package="0402-RES" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="Protofusion-passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Protofusion-passives" package="0805-CAP" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Protofusion-passives" package="0805-CAP" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Protofusion-passives" package="0402-RES" value="2M 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Protofusion-passives" package="0402-RES" value="2M 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="Protofusion-passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="Protofusion-passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Protofusion-passives" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="Protofusion-passives" package="0402-CAP" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SLAT-Analog" package="ASDM" value="ASDMB-26.000MHZ-LY-T ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Protofusion-passives" package="0402-RES" value="100k"/>
<element name="R3" library="Protofusion-passives" package="0603-RES" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Protofusion-passives" package="0402-RES" value="4.7k"/>
<element name="R10" library="Protofusion-passives" package="0402-RES" value="4.7k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="18"/>
<contactref element="U7" pad="12_GND"/>
<contactref element="U7" pad="10_GND"/>
<contactref element="U7" pad="1_GND"/>
<contactref element="U6" pad="16"/>
<contactref element="J1" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="GND-1" pad="1"/>
<contactref element="GND-2" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="9"/>
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="5"/>
<contactref element="CM2" pad="2"/>
<contactref element="CM1" pad="2"/>
<contactref element="CM" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="6"/>
<contactref element="U6" pad="17"/>
<contactref element="U6" pad="5"/>
<contactref element="U7" pad="6_V_BCKP"/>
<contactref element="J1" pad="1"/>
<contactref element="U4" pad="3"/>
<contactref element="LCHOKE" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="R10" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U5" pad="10"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="RADIO-GPIO1">
<contactref element="U1" pad="10"/>
<contactref element="U6" pad="20"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RADIO-SHDN">
<contactref element="U1" pad="1"/>
<contactref element="U6" pad="19"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="4"/>
<contactref element="C0" pad="2"/>
<contactref element="LCHOKE" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C0" pad="1"/>
<contactref element="L0" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="CM" pad="1"/>
<contactref element="L0" pad="1"/>
<contactref element="LM1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="CM1" pad="1"/>
<contactref element="LM1" pad="1"/>
<contactref element="LM2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="17"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="GPSVCC">
<contactref element="U7" pad="9_V_RESET"/>
<contactref element="U7" pad="8_VCC"/>
<contactref element="U7" pad="7_VCC_IO"/>
<contactref element="Q2" pad="3"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="GPS_EN_GATE">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="GPS_FEED">
<contactref element="U7" pad="11_RF_IN"/>
<contactref element="U2" pad="FEED"/>
</signal>
<signal name="TIMEPULSE">
<contactref element="U7" pad="4_TIMEPULSE"/>
</signal>
<signal name="GPS-RX">
<contactref element="U7" pad="3_RXD1"/>
<contactref element="U6" pad="8"/>
</signal>
<signal name="GPS-TX">
<contactref element="U7" pad="2_TXD1"/>
<contactref element="U6" pad="9"/>
</signal>
<signal name="GPS-EN">
<contactref element="U6" pad="7"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="RADIO-MOSI">
<contactref element="U6" pad="26"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="RADIO-MISO">
<contactref element="U6" pad="25"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="RADIO-SCK">
<contactref element="U6" pad="24"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="RADIO-NSS">
<contactref element="U6" pad="23"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="SWCLK">
<contactref element="U6" pad="22"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SWDIO">
<contactref element="U6" pad="21"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="L1" pad="2"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="LED">
<contactref element="U6" pad="14"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="VBATT_SENSE">
<contactref element="U6" pad="12"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="VBATT">
<contactref element="U4" pad="5"/>
<contactref element="U4" pad="4"/>
<contactref element="J3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="TCXO-EN">
<contactref element="U6" pad="18"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U5" pad="4"/>
<contactref element="U6" pad="28"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U6" pad="27"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="ANT" pad="1"/>
<contactref element="LM3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="CM2" pad="1"/>
<contactref element="LM2" pad="1"/>
<contactref element="LM3" pad="2"/>
</signal>
<signal name="OSC_OUT">
<contactref element="U3" pad="3"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$16">
</signal>
<signal name="SCL-FLIP">
<contactref element="U5" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$19">
</signal>
</signals>
</board>
</drawing>
</eagle>
