<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="10.922" y1="9.906" x2="25.324" y2="9.906" width="0" layer="20"/>
<wire x1="25.324" y1="9.906" x2="25.324" y2="21.834" width="0" layer="20"/>
<wire x1="25.324" y1="21.834" x2="10.922" y2="21.834" width="0" layer="20"/>
<wire x1="10.922" y1="21.834" x2="10.922" y2="9.906" width="0" layer="20"/>
<text>Crappy 1040 MPPT
Test Board r01</text>
<text>vcap</text>
<text>gnd</text>
<text>gnd</text>
<text>vsol</text>
</plain>
<libraries>
<library name="PecanPico6">
<description>Generated from &lt;b&gt;PecanPico6.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="TSSOP8">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1210">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SLAT-RCL">
<description>SLAT Resisters, Capacitors, Inductors</description>
<packages>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="0805-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SLAT-RCL" package="0603-CAP" value="1nF">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SLAT-RCL" package="0805-CAP" value="22uF">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SLAT-RCL" package="0805-CAP" value="10uF">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="PecanPico6" package="TSSOP8" value="SPV1040T">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SLAT-RCL" package="0603-RES" value="22k">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SLAT-RCL" package="0603-RES" value="10k">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="1210" value="LQH32CN100K33L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VBATT" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="GND1" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="GND2" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="VSOL" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="GND1" pad="TP"/>
<contactref element="GND2" pad="TP"/>
</signal>
<signal name="VBAT">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="VBATT" pad="TP"/>
</signal>
<signal name="VSOLAR">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="C2" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="VSOL" pad="TP"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="3"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
