{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["wsprhab-flex"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"wsprhab-flex","index":0,"n_rows":21,"n_cols":11,"rows_kept":21,"flags":["formulas_cached_only"]}
["Qty","Value","Device","Package","Parts","Description","DIGIKEY_PART_NUMBER","MANUFACTURER","PART_NUMBER","TOLERANCE","VOLTAGE"]
[8,"0.1uF","CAPACITOR0402","0402-CAP","C3, C5, C6, C9, C10, C12, C14, C15","Ceramic capacitor",null,"Murata Electronics","GRM155R62A104KE14D"]
[2,"10K","RESISTOR0402","0402-RES","R2, R3","Chip resistor",null,"Panasonic Electronic Components","ERJ-2GEJ103X"]
[2,"10uF","CAPACITOR0603","0603-CAP","C1, C4","Ceramic capacitor",null,"Murata Electronics","GRM188R61A106KE69J",null,"10V"]
[1,"10uH","INDUCTOR0603","0603-INDUCTOR","L2","Inductor",null,"TDK Corporation","MLZ1608N100LT000"]
[1,"10uH","INDUCTOR1008","1008-INDUCTOR","L1","Inductor",null,"Delta Electronics/Cyntec","HTEX25201B-100MSR"]
[1,"15F","CAP-POLAR","MAL219691204E3","C8",null,null,"Vishay BC Components","MAL219691203E3"]
[2,"1uF","CAPACITOR0402","0402-CAP","C16, C17","Ceramic capacitor",null,"Samsung Electro-Mechanics","CL05A105KP5NNNC"]
[1,"22uF","CAPACITOR0603","0603-CAP","C2","Ceramic capacitor",null,"Samsung Electro-Mechanics","CL10A226MPMNUBE",null,"10V"]
[2,"423pF","CAPACITOR0402","0402-CAP","C11, C13","Ceramic capacitor",null,"Taiyo Yuden","UMK105CH431JVHF"]
[1,510,"RESISTOR0402","0402-RES","R1","Chip resistor",null,"Panasonic Electronic Components","ERJ-2GEJ511X"]
[1,"720nH","INDUCTOR0402","0402-INDUCTOR","L3","Inductor",null,"Taiyo Yuden","BRC1608TR72M6"]
[1,"AEM10941","AEM10941","QFN50P505X505X90-28","U1","Ambient Energy Manager from e-peas",null,"e-peas","AEM10941"]
[1,"CONN-2JST-ZH-2-VERT","CONN-2JST-ZH-2-VERT","JST_ZH-V-2-1","J1","2 position header",null,"JST Sales America Inc.","B2B-ZR(LF)(SN)"]
[1,"GPS_ANTENNA","GPS_ANTENNA","AVA_JTI_ANTENNA-1575AT43A40","RF1",null,null,"Johanson Technology Inc.","1575AT43A0040E"]
[1,"Green","LED0603","LED-0603","D1","Single LED chip",null,"Wurth Elektronik","150060VS75000"]
[1,"SI5351C","SI5351C","QFN20-4X4","U4","Clock generator 8 output with VCO",null,"Silicon Labs","SI5351C-B-GMR"]
[1,"STM32L031G6U6","STM32L031G6U6","UFQFPN28","U2",null,null,"STMicroelectronics","STM32L031G6U6"]
[1,"TCR2EE","TCR2EE","SOT-553","U6",null,null,"Toshiba Semiconductor and Storage","TCR2EE33,LM(CT"]
[1,"TCXOABRACON","TCXOABRACON","ASTX-H11","U5",null,null,"Abracon","ASTX-H11-B-10.000MHZ-I25-T"]
[1,"UBLOX_MAX-8","UBLOX_MAX-8","UBLOX_MAX-8","U3","UBLOX MAX-8",null,"U-Blox","MAX-M8Q-0-10"]