<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<packages>
<package name="SOP4">
</package>
<package name="RJ45-8_SMD-1">
</package>
<package name="0603-ARV-4">
</package>
<package name="RJ45-8_SMD-2">
</package>
<package name="TSSOP16">
</package>
<package name="LED-SMD-10W-DX">
</package>
<package name="LED-SMD-10W-DX-W_POUR">
</package>
<package name="SOT23-5">
</package>
<package name="SRN6045">
</package>
<package name="2X3-PINHEADER-SMT">
</package>
<package name="POGOPROG-BACKMOUNT">
</package>
<package name="POGOPROG-CONN">
<description>Standard pogo pin programming header with two alignment holes. Small SMD pads.</description>
</package>
<package name="POGOPROG-CONN-W">
<description>Standard pogo pin programming header with two alignment holes. WIDE smd pads.</description>
</package>
<package name="POGOPROG-CONN-1H">
<description>Standard pogo pin programming header with ONE alignment hole. Small SMD pads.</description>
</package>
<package name="POGOPROG-CONN-0H">
<description>No holes, 2 vias, pogo pin programming header.</description>
</package>
<package name="POGOPROG-CONN-OH-SMALLERVIAS">
<description>No holes, 2 vias, pogo pin programming header. With smaller vias.</description>
</package>
<package name="POGOPROG-CONN-OH-1V">
<description>No holes, 1 via, pogo pin programming header.</description>
</package>
<package name="LED-SMD-10W-DX-STOPONLY">
</package>
<package name="LZ4">
</package>
<package name="MSOP-8_POWERPAD">
</package>
<package name="LED-700MA-1CH">
</package>
<package name="TQFP64">
</package>
<package name="POGOPROG-CONN-ALLSMT">
</package>
<package name="UFQFPN32">
</package>
<package name="1206-ARV-4">
</package>
<package name="LQFP32">
</package>
<package name="UFQFPN28">
</package>
<package name="POGOPROG-CONN-4-ALLSMT">
</package>
<package name="CRYSTAL-3.2X2.5">
</package>
<package name="TSOT23-6">
</package>
<package name="SO8">
</package>
<package name="SOT363">
</package>
<package name="JOHANSON-TECH_ANTENNA_915MHZ">
</package>
<package name="LAIRD_BMI-S-101">
</package>
<package name="LQFP48">
</package>
<package name="QFN20">
</package>
<package name="QFN20-5X5">
</package>
<package name="POGOPROG-BACKMOUNT-SWD">
</package>
<package name="VFQFPN20-3X3">
</package>
<package name="SC70JW-8">
</package>
<package name="WIREPAD">
</package>
<package name="SF1186G">
<description>Package for SF1186G SAW filter</description>
</package>
<package name="SOT23-6">
</package>
<package name="SOIC8">
<description>SOIC8 package type.</description>
</package>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SOT323-R">
<description>&lt;b&gt;SOT323 Reflow soldering&lt;/b&gt;&lt;p&gt;
Philips SC01_Mounting_1996.pdf</description>
</package>
<package name="TSX-3225">
<description>Footprint for TSX-3225 Crystal</description>
</package>
<package name="PTC-1206">
</package>
<package name="ABM8G">
</package>
<package name="BANANA-PCB-HOR-TH">
</package>
<package name="FIDUCIAL-1.5X3">
</package>
<package name="SMB">
<description>&lt;b&gt;Diode&lt;/b&gt;&lt;p&gt;
SMB footprint. Diode polarity has been removed for bi-directional parts.</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="VOM1271">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="STM32F302X">
<pin name="VDD1" direction="pwr"/>
<pin name="PF0/OSC_IN"/>
<pin name="PF1/OSC_OUT"/>
<pin name="NRST"/>
<pin name="VDDA/VREF+" direction="pwr"/>
<pin name="VSSA/VREF-" direction="sup"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="VSS2" direction="sup"/>
<pin name="VDD2" direction="pwr"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="SWDIO/PA13"/>
<pin name="SWCLK/PA14"/>
<pin name="PA15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT0"/>
<pin name="VSS1" direction="sup"/>
<pin name="PAD" direction="sup"/>
</symbol>
<symbol name="RJ45-8">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="GND0"/>
<pin name="GND1"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="STP04CM05XTTR">
<description>Linear LED Driver (UNPROVEN!)</description>
<pin name="VCC"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
<pin name="OUT0"/>
<pin name="NOE"/>
<pin name="GND"/>
<pin name="SDO"/>
<pin name="REXT"/>
</symbol>
<symbol name="LED-RGB">
<pin name="R-" direction="pas"/>
<pin name="R+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="B-" direction="pas"/>
<pin name="B+" direction="pas"/>
</symbol>
<symbol name="AL8805">
<pin name="SW"/>
<pin name="GND"/>
<pin name="CTRL"/>
<pin name="VIN"/>
<pin name="SET"/>
</symbol>
<symbol name="LED">
<pin name="R-" direction="pas"/>
<pin name="R+" direction="pas"/>
</symbol>
<symbol name="L">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="AVR-ISP">
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="\RST"/>
<pin name="VTG"/>
<pin name="MOSI"/>
<pin name="GND"/>
</symbol>
<symbol name="POGOPROG-BACKBOARD">
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="\RST"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="BODY1"/>
<pin name="BODY2"/>
</symbol>
<symbol name="POGOPROG-CONN">
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="\RST"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="LED-LZ4-RGBW">
<pin name="B+"/>
<pin name="B-"/>
<pin name="R+"/>
<pin name="R-"/>
<pin name="G+"/>
<pin name="G-"/>
<pin name="W+"/>
<pin name="W-"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="AUDIO-AMP-MONO-3.1W">
<pin name="SHUTDOWN"/>
<pin name="BYPASS"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="VO+"/>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="VO-"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="STM32L100">
<pin name="VLCD" direction="pwr"/>
<pin name="PC13"/>
<pin name="PC14/OSC32_IN"/>
<pin name="PC15/OSC32_OUT"/>
<pin name="PH0/OSC_IN" direction="in"/>
<pin name="PH1/OSC_OUT" direction="out"/>
<pin name="NRST"/>
<pin name="PC0/ADC10"/>
<pin name="PC1/ADC11"/>
<pin name="PC2/ADC12"/>
<pin name="PC3/ADC13"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PA0/WKUP1"/>
<pin name="PA1/ADC0"/>
<pin name="PA2/UART2_TX/ADC1"/>
<pin name="PA3/UART2_RX/ADC2"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="PA4/SPI1_NSS/ADC4/DAC1"/>
<pin name="PA5/SPI1_SCK/ADC5/DAC2"/>
<pin name="PA6/SPI1_MISO/ADC6"/>
<pin name="PA7/SPI1_MOSI/ADC7"/>
<pin name="PC4/ADC14"/>
<pin name="PC5/ADC15"/>
<pin name="PB0/ADC8"/>
<pin name="PB1/ADC9"/>
<pin name="PB2/BOOT1"/>
<pin name="PB10/I2C2_SCL/UART3_TX"/>
<pin name="PB11/I2C2_SDA/UART3_RX"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="I2C2_SMBA/ADC18/PB12"/>
<pin name="SPI2_SCK/ADC19/PB13"/>
<pin name="SPI2_MISO/ADC20/PB14"/>
<pin name="SPI2_MOSI/ADC21/PB15"/>
<pin name="I2S2_MCK/PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PA8"/>
<pin name="UART1_TX/PA9"/>
<pin name="UART1_RX/PA10"/>
<pin name="USB_DM/SPI1_MISO/PA11"/>
<pin name="USB_DP/SPI1_MOSI/PA12"/>
<pin name="JTMS/SWDIO/PA13"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="JTCK/SWCLK/PA14"/>
<pin name="JTDI/PA15"/>
<pin name="UART3_TX/PC10"/>
<pin name="UART3_RX/PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="JTDO/PB3"/>
<pin name="NJTRST/SPI1_MISO/PB4"/>
<pin name="I2C1_SMBA/SPI1_MOSI/PB5"/>
<pin name="I2C1_SCL/UART1_TX/PB6"/>
<pin name="I2C1_SDA/UART1_RX/PB7"/>
<pin name="BOOT0" direction="in"/>
<pin name="I2C1_SCL/PB8"/>
<pin name="I2C1_SDA/PB9"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
</symbol>
<symbol name="STM32F042K-U">
<pin name="VDD"/>
<pin name="PF0/I2C1_SDA"/>
<pin name="PF1/I2C1_SCL"/>
<pin name="NRST"/>
<pin name="VDDA"/>
<pin name="PA0/ADC0"/>
<pin name="PA1/ADC1"/>
<pin name="PA2/ADC2/USART2_TX"/>
<pin name="PA3/ADC3/USART2_RX"/>
<pin name="PA4/ADC4"/>
<pin name="PA5/ADC5/SPI1_SCK"/>
<pin name="PA6/ADC6/SPI1_MISO"/>
<pin name="PA7/ADC7/SPI1_MOSI"/>
<pin name="PB0/ADC8"/>
<pin name="PB1/ADC9"/>
<pin name="PB2"/>
<pin name="VDDIO2"/>
<pin name="PA8"/>
<pin name="USART1_TX/I2C1_SCL/PA9"/>
<pin name="USART1_RX/I2C1_SDA/PA10"/>
<pin name="CAN_RX/I2C1_SCL/USB_DM/PA11"/>
<pin name="CAN_TX/I2C1_SDA/USB_DP/PA12"/>
<pin name="SWDIO/PA13"/>
<pin name="USART2_TX/SWCLK/PA14"/>
<pin name="USART2_RX/PA15"/>
<pin name="SPI1_SCK/PB3"/>
<pin name="SPI1_MISO/PB4"/>
<pin name="SPI1_MOSI/PB5"/>
<pin name="I2C1_SCL/USART1_TX/PB6"/>
<pin name="I2C1_SDA/USART1_RX/PB7"/>
<pin name="BOOT0-PF11"/>
<pin name="I2C1_SCL/CAN_RX/PB8"/>
<pin name="GND"/>
</symbol>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="STM32F042K-T">
<pin name="VDD"/>
<pin name="PF0/I2C1_SDA"/>
<pin name="PF1/I2C1_SCL"/>
<pin name="NRST"/>
<pin name="VDDA"/>
<pin name="PA0/ADC0"/>
<pin name="PA1/ADC1"/>
<pin name="PA2/ADC2/USART2_TX"/>
<pin name="PA3/ADC3/USART2_RX"/>
<pin name="PA4/ADC4"/>
<pin name="PA5/ADC5/SPI1_SCK"/>
<pin name="PA6/ADC6/SPI1_MISO"/>
<pin name="PA7/ADC7/SPI1_MOSI"/>
<pin name="PB0/ADC8"/>
<pin name="PB1/ADC9"/>
<pin name="VDDIO2"/>
<pin name="PA8"/>
<pin name="USART1_TX/I2C1_SCL/PA9"/>
<pin name="USART1_RX/I2C1_SDA/PA10"/>
<pin name="CAN_RX/I2C1_SCL/USB_DM/PA11"/>
<pin name="CAN_TX/I2C1_SDA/USB_DP/PA12"/>
<pin name="SWDIO/PA13"/>
<pin name="USART2_TX/SWCLK/PA14"/>
<pin name="USART2_RX/PA15"/>
<pin name="SPI1_SCK/PB3"/>
<pin name="SPI1_MISO/PB4"/>
<pin name="SPI1_MOSI/PB5"/>
<pin name="I2C1_SCL/USART1_TX/PB6"/>
<pin name="I2C1_SDA/USART1_RX/PB7"/>
<pin name="BOOT0/I2C1_SCL/CAN_RX/PB8"/>
<pin name="GND"/>
</symbol>
<symbol name="STM32F031G6U6">
<pin name="BOOT0"/>
<pin name="PF0/OSC_IN"/>
<pin name="PF1/OSC_OUT"/>
<pin name="NRST"/>
<pin name="VDDA"/>
<pin name="PA0"/>
<pin name="PA1/TIM2_2"/>
<pin name="PA2/TIM2_3/USART1_TX"/>
<pin name="PA3/TIM2_4/USART1_RX"/>
<pin name="PA4/SPI1_NSS/TIM14_1"/>
<pin name="PA5/SPI1_SCK"/>
<pin name="PA6/SPI1_MISO/TIM3_1"/>
<pin name="PA7/SPI1_MOSI/TIM3_2"/>
<pin name="PB0/TIM3_3"/>
<pin name="PB1/TIM3_4"/>
<pin name="VSS"/>
<pin name="TIM1_1/MCO/PA8"/>
<pin name="UART1_TX/TIM1_2/I2C1_SCL/PA9"/>
<pin name="USART1_TX/TIM1_3/I2C1_SDA/PA10"/>
<pin name="SWDIO/PA13"/>
<pin name="USART1_TX/SWCLK/PA14"/>
<pin name="SPI1_NSS/USART1_RX/PA15"/>
<pin name="SPI1_SCK/TIM2_2/PB3"/>
<pin name="SPI1_MISO/TIM3_1/PB4"/>
<pin name="SPI1_MOSI/TIM3_2/PB5"/>
<pin name="I2C1_SCL/USART1_TX/PB6"/>
<pin name="I2C1_SDA/USART1_RX/PB7"/>
<pin name="VDD"/>
</symbol>
<symbol name="POGOPROG-CONN-4">
<pin name="SWDIO"/>
<pin name="SWCLK"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="TXVCO">
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="CNTRL" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="LTC3531">
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="GND"/>
<pin name="VOUT"/>
<pin name="!SHDN"/>
<pin name="VIN"/>
</symbol>
<symbol name="UPG2214TB">
<pin name="VC1"/>
<pin name="RF_IN"/>
<pin name="VC2"/>
<pin name="OUT2"/>
<pin name="GND"/>
<pin name="OUT1"/>
</symbol>
<symbol name="ANTENNA">
<pin name="ANTENNA" direction="in"/>
</symbol>
<symbol name="SHIELD">
<pin name="SHIELD"/>
</symbol>
<symbol name="STM32F042C6T6">
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDDA"/>
<pin name="VDDAIO"/>
<pin name="VBAT"/>
<pin name="NRST"/>
<pin name="PF0/OSC-IN"/>
<pin name="PF1/OSC_OUT"/>
<pin name="PF11/BOOT0"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="PA0\"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
</symbol>
<symbol name="MAX31865">
<description>&lt;b&gt;RTD to Digital Converter&lt;/b&gt;&lt;br /&gt;&lt;br /&gt;

The MAX31865 is a -to-digital 
converter optimized for platinum resistance temperature 
detectors (RTDs).&lt;br /&gt;&lt;br /&gt;

An external resistor sets the sensitivity 
for the RTD being used and a delta-sigma ADC 
converts the ratio of the RTD resistance to the reference 
resistance into digital form. The MAX31865???s inputs are 
protected against overvoltage faults of up to +/-50V. 
Programmable detection of RTD and cable open and 
short conditions is included.</description>
<pin name="!DRDY" direction="out"/>
<pin name="SDI" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="BIAS" direction="in"/>
<pin name="REFIN+" direction="in"/>
<pin name="REFIN-" direction="in"/>
<pin name="ISENSOR" direction="in"/>
<pin name="FORCE+" direction="in"/>
<pin name="FORCE2" direction="in"/>
<pin name="RTDIN+" direction="in"/>
<pin name="RTDIN-" direction="in"/>
<pin name="FORCE-" direction="in"/>
</symbol>
<symbol name="SPV1050">
<pin name="IN_LV"/>
<pin name="IN_HV"/>
<pin name="L_HV"/>
<pin name="MPP"/>
<pin name="MPP_SET"/>
<pin name="MPP_REF"/>
<pin name="LDO1_EN"/>
<pin name="LDO2_EN"/>
<pin name="CONF"/>
<pin name="PGND"/>
<pin name="GND"/>
<pin name="BATT_CHG"/>
<pin name="BATT_CON"/>
<pin name="LDO2"/>
<pin name="LDO1"/>
<pin name="EOC"/>
<pin name="UVP"/>
<pin name="STORE"/>
<pin name="BATT"/>
</symbol>
<symbol name="WIREPAD">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="AAT3681A">
<description>AAT3681A Lipo battery charging ic</description>
<pin name="ADP"/>
<pin name="EN"/>
<pin name="STAT"/>
<pin name="BAT"/>
<pin name="ISET"/>
<pin name="GND"/>
</symbol>
<symbol name="SF1186G">
<description>Symbol for SF1186G SAW filter</description>
<pin name="IN"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="AOZ1282CI">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="FB"/>
<pin name="LX"/>
<pin name="BS"/>
</symbol>
<symbol name="SN65HVD234">
<pin name="CANH"/>
<pin name="CANL"/>
<pin name="D"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="R"/>
<pin name="RS"/>
<pin name="VCC"/>
</symbol>
<symbol name="PESD1CAN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="MCP16301">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="BOOST"/>
<pin name="SW"/>
<pin name="FB"/>
</symbol>
<symbol name="CRYSTAL">
<description>Crystal symbol</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="PTC">
<description>PTC Fuse</description>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="BANANA-CONN">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MOSFET-N">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="MOSFET-P">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="ACS7XX">
<pin name="IP+" direction="pas"/>
<pin name="IP-" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="VIOUT" direction="pas"/>
<pin name="!FAULT" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="DIODE-TVS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="OPAMP_2">
<pin name="-IN1" direction="in"/>
<pin name="+IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="+V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OPAMP_2_1">
<pin name="OUT2" direction="out"/>
<pin name="-IN2" direction="in"/>
<pin name="+IN2" direction="in"/>
</symbol>
<symbol name="OK">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="EMIT" direction="pas"/>
<pin name="COL" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VOM1271" prefix="U">
<description>&lt;p&gt; Vishay - Photovoltaic MOSFET Driver  &lt;p&gt;&lt;be&gt;

&lt;p&gt;&lt;b&gt;Manufacturer:&lt;/b&gt; Vishay Semiconductor &lt;p&gt;&lt;be&gt;

&lt;p&gt;&lt;b&gt;Description:&lt;/b&gt; OPTOISOLATOR 4.5KV PHVOLT 4-SOP &lt;p&gt;&lt;be&gt;

&lt;p&gt;&lt;b&gt;Manufacturer Part Number:&lt;/b&gt; VOM1271T &lt;p&gt;&lt;be&gt;

&lt;a href="http://www.digikey.com/product-detail/en/VOM1271T/VOM1271TCT-ND/3588699"&gt;Digi-Key&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="VOM1271"/>
</gates>
<devices>
<device name="" package="SOP4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F302X" prefix="U">
<gates>
<gate name="G$1" symbol="STM32F302X"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="G$1" pin="BOOT0" pad="31"/>
<connect gate="G$1" pin="NRST" pad="4"/>
<connect gate="G$1" pin="PA0" pad="7"/>
<connect gate="G$1" pin="PA1" pad="8"/>
<connect gate="G$1" pin="PA10" pad="20"/>
<connect gate="G$1" pin="PA11" pad="21"/>
<connect gate="G$1" pin="PA12" pad="22"/>
<connect gate="G$1" pin="PA15" pad="25"/>
<connect gate="G$1" pin="PA2" pad="9"/>
<connect gate="G$1" pin="PA3" pad="10"/>
<connect gate="G$1" pin="PA4" pad="11"/>
<connect gate="G$1" pin="PA5" pad="12"/>
<connect gate="G$1" pin="PA6" pad="13"/>
<connect gate="G$1" pin="PA7" pad="14"/>
<connect gate="G$1" pin="PA8" pad="18"/>
<connect gate="G$1" pin="PA9" pad="19"/>
<connect gate="G$1" pin="PAD" pad="EXP"/>
<connect gate="G$1" pin="PB0" pad="15"/>
<connect gate="G$1" pin="PB3" pad="26"/>
<connect gate="G$1" pin="PB4" pad="27"/>
<connect gate="G$1" pin="PB5" pad="28"/>
<connect gate="G$1" pin="PB6" pad="29"/>
<connect gate="G$1" pin="PB7" pad="30"/>
<connect gate="G$1" pin="PF0/OSC_IN" pad="2"/>
<connect gate="G$1" pin="PF1/OSC_OUT" pad="3"/>
<connect gate="G$1" pin="SWCLK/PA14" pad="24"/>
<connect gate="G$1" pin="SWDIO/PA13" pad="23"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="17"/>
<connect gate="G$1" pin="VDDA/VREF+" pad="5"/>
<connect gate="G$1" pin="VSS1" pad="32"/>
<connect gate="G$1" pin="VSS2" pad="16"/>
<connect gate="G$1" pin="VSSA/VREF-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45">
<description>&lt;b&gt;RJ45 Jack&lt;/b&gt;
Simple RJ45, 8-pin connection - connector for common Cat5, Cat5e, and Cat6 Ethernet cables. 
&lt;br&gt;&lt;br&gt;
MOLEX SMD P/N: 43743-8101</description>
<gates>
<gate name="G$1" symbol="RJ45-8"/>
</gates>
<devices>
<device name="BIGPKG" package="RJ45-8_SMD-1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="GND0" pad="P$9"/>
<connect gate="G$1" pin="GND1" pad="P$10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALLPKG" package="RJ45-8_SMD-2">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="GND0" pad="P$9"/>
<connect gate="G$1" pin="GND1" pad="P$10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-ARRAY">
<gates>
<gate name="A" symbol="RESISTOR"/>
<gate name="B" symbol="RESISTOR"/>
<gate name="C" symbol="RESISTOR"/>
<gate name="D" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="0603-ARV-4">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STP04CM05XTTR">
<description>Linear LED Driver (UNPROVEN!)</description>
<gates>
<gate name="G$1" symbol="STP04CM05XTTR"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="GND" pad="1 2"/>
<connect gate="G$1" pin="LE" pad="5"/>
<connect gate="G$1" pin="NOE" pad="13"/>
<connect gate="G$1" pin="OUT0" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="REXT" pad="15"/>
<connect gate="G$1" pin="SDI" pad="3"/>
<connect gate="G$1" pin="SDO" pad="14"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-10W">
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="PAD" package="LED-SMD-10W-DX">
<connects>
<connect gate="G$1" pin="B+" pad="B+"/>
<connect gate="G$1" pin="B-" pad="B-"/>
<connect gate="G$1" pin="G+" pad="G+"/>
<connect gate="G$1" pin="G-" pad="G-"/>
<connect gate="G$1" pin="R+" pad="R+"/>
<connect gate="G$1" pin="R-" pad="R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AL8805">
<description>DC/DC constant-current buck for driving LEDs (up to 1A)</description>
<gates>
<gate name="G$1" symbol="AL8805"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CTRL" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SET" pad="4"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-10W-MODULAR">
<gates>
<gate name="RED" symbol="LED"/>
<gate name="GREEN" symbol="LED"/>
<gate name="BLUE" symbol="LED"/>
</gates>
<devices>
<device name="WITHCOPPER" package="LED-SMD-10W-DX">
<connects>
<connect gate="BLUE" pin="R+" pad="B+"/>
<connect gate="BLUE" pin="R-" pad="B-"/>
<connect gate="GREEN" pin="R+" pad="G+"/>
<connect gate="GREEN" pin="R-" pad="G-"/>
<connect gate="RED" pin="R+" pad="R+"/>
<connect gate="RED" pin="R-" pad="R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="STOPONLY" package="LED-SMD-10W-DX-STOPONLY">
<connects>
<connect gate="BLUE" pin="R+" pad="B+"/>
<connect gate="BLUE" pin="R-" pad="B-"/>
<connect gate="GREEN" pin="R+" pad="G+"/>
<connect gate="GREEN" pin="R-" pad="G-"/>
<connect gate="RED" pin="R+" pad="R+"/>
<connect gate="RED" pin="R-" pad="R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRN6045">
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="SRN6045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-ISP">
<gates>
<gate name="G$1" symbol="AVR-ISP"/>
</gates>
<devices>
<device name="" package="2X3-PINHEADER-SMT">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VTG" pad="2"/>
<connect gate="G$1" pin="\RST" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POGOPIN-BACKBOARD">
<gates>
<gate name="G$1" symbol="POGOPROG-BACKBOARD"/>
</gates>
<devices>
<device name="" package="POGOPROG-BACKMOUNT">
<connects>
<connect gate="G$1" pin="BODY1" pad="1"/>
<connect gate="G$1" pin="BODY2" pad="8"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MISO" pad="5"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="\RST" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POGOPIN-CONN">
<description>Protofusion custom pogo pin programming header</description>
<gates>
<gate name="J" symbol="POGOPROG-CONN"/>
</gates>
<devices>
<device name="STANDARD" package="POGOPROG-CONN">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS" package="POGOPROG-CONN-0H">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ONEHOLE" package="POGOPROG-CONN-1H">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS-SMV" package="POGOPROG-CONN-OH-SMALLERVIAS">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="POGOPROG-CONN-W">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS-1V" package="POGOPROG-CONN-OH-1V">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ALLSMT" package="POGOPROG-CONN-ALLSMT">
<connects>
<connect gate="J" pin="GND" pad="2"/>
<connect gate="J" pin="MISO" pad="4"/>
<connect gate="J" pin="MOSI" pad="5"/>
<connect gate="J" pin="SCK" pad="3"/>
<connect gate="J" pin="VCC" pad="1"/>
<connect gate="J" pin="\RST" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZ4-RGBW">
<gates>
<gate name="G$1" symbol="LED-LZ4-RGBW"/>
</gates>
<devices>
<device name="" package="LZ4">
<connects>
<connect gate="G$1" pin="B+" pad="7"/>
<connect gate="G$1" pin="B-" pad="8"/>
<connect gate="G$1" pin="G+" pad="5"/>
<connect gate="G$1" pin="G-" pad="6"/>
<connect gate="G$1" pin="R+" pad="3"/>
<connect gate="G$1" pin="R-" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20 P$21 P$22 P$23 P$24 P$25 P$26 P$27 P$28 P$29 P$30 P$31 P$32 P$33 P$34 P$35 P$36 P$37 P$38 P$39 THERMAL"/>
<connect gate="G$1" pin="W+" pad="1"/>
<connect gate="G$1" pin="W-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZ4-RGBW-FLAT" package="LZ4">
<connects>
<connect gate="G$1" pin="B+" pad="2"/>
<connect gate="G$1" pin="B-" pad="7"/>
<connect gate="G$1" pin="G+" pad="1"/>
<connect gate="G$1" pin="G-" pad="8"/>
<connect gate="G$1" pin="R+" pad="3"/>
<connect gate="G$1" pin="R-" pad="6"/>
<connect gate="G$1" pin="THERMAL" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20 P$21 P$22 P$23 P$24 P$25 P$26 P$27 P$28 P$29 P$30 P$31 P$32 P$33 P$34 P$35 P$36 P$37 P$38 P$39 THERMAL"/>
<connect gate="G$1" pin="W+" pad="4"/>
<connect gate="G$1" pin="W-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO-AMP-MONO-3.1W">
<description>Part No.: TPA6211A1TDGNRQ1</description>
<gates>
<gate name="G$1" symbol="AUDIO-AMP-MONO-3.1W"/>
</gates>
<devices>
<device name="" package="MSOP-8_POWERPAD">
<connects>
<connect gate="G$1" pin="BYPASS" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="SHUTDOWN" pad="1"/>
<connect gate="G$1" pin="THERMAL" pad="T1 T2 T3 T4 T5 T6"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VO+" pad="5"/>
<connect gate="G$1" pin="VO-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED-700MA-1CH">
<connects>
<connect gate="G$1" pin="R+" pad="ANODE THERMAL"/>
<connect gate="G$1" pin="R-" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L100">
<description>IC MCU 32BIT 128KB FLASH 64LQFP</description>
<gates>
<gate name="G$1" symbol="STM32L100"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="G$1" pin="BOOT0" pad="60"/>
<connect gate="G$1" pin="I2C1_SCL/PB8" pad="61"/>
<connect gate="G$1" pin="I2C1_SCL/UART1_TX/PB6" pad="58"/>
<connect gate="G$1" pin="I2C1_SDA/PB9" pad="62"/>
<connect gate="G$1" pin="I2C1_SDA/UART1_RX/PB7" pad="59"/>
<connect gate="G$1" pin="I2C1_SMBA/SPI1_MOSI/PB5" pad="57"/>
<connect gate="G$1" pin="I2C2_SMBA/ADC18/PB12" pad="33"/>
<connect gate="G$1" pin="I2S2_MCK/PC6" pad="37"/>
<connect gate="G$1" pin="JTCK/SWCLK/PA14" pad="49"/>
<connect gate="G$1" pin="JTDI/PA15" pad="50"/>
<connect gate="G$1" pin="JTDO/PB3" pad="55"/>
<connect gate="G$1" pin="JTMS/SWDIO/PA13" pad="46"/>
<connect gate="G$1" pin="NJTRST/SPI1_MISO/PB4" pad="56"/>
<connect gate="G$1" pin="NRST" pad="7"/>
<connect gate="G$1" pin="PA0/WKUP1" pad="14"/>
<connect gate="G$1" pin="PA1/ADC0" pad="15"/>
<connect gate="G$1" pin="PA2/UART2_TX/ADC1" pad="16"/>
<connect gate="G$1" pin="PA3/UART2_RX/ADC2" pad="17"/>
<connect gate="G$1" pin="PA4/SPI1_NSS/ADC4/DAC1" pad="20"/>
<connect gate="G$1" pin="PA5/SPI1_SCK/ADC5/DAC2" pad="21"/>
<connect gate="G$1" pin="PA6/SPI1_MISO/ADC6" pad="22"/>
<connect gate="G$1" pin="PA7/SPI1_MOSI/ADC7" pad="23"/>
<connect gate="G$1" pin="PA8" pad="41"/>
<connect gate="G$1" pin="PB0/ADC8" pad="26"/>
<connect gate="G$1" pin="PB1/ADC9" pad="27"/>
<connect gate="G$1" pin="PB10/I2C2_SCL/UART3_TX" pad="29"/>
<connect gate="G$1" pin="PB11/I2C2_SDA/UART3_RX" pad="30"/>
<connect gate="G$1" pin="PB2/BOOT1" pad="28"/>
<connect gate="G$1" pin="PC0/ADC10" pad="8"/>
<connect gate="G$1" pin="PC1/ADC11" pad="9"/>
<connect gate="G$1" pin="PC12" pad="53"/>
<connect gate="G$1" pin="PC13" pad="2"/>
<connect gate="G$1" pin="PC14/OSC32_IN" pad="3"/>
<connect gate="G$1" pin="PC15/OSC32_OUT" pad="4"/>
<connect gate="G$1" pin="PC2/ADC12" pad="10"/>
<connect gate="G$1" pin="PC3/ADC13" pad="11"/>
<connect gate="G$1" pin="PC4/ADC14" pad="24"/>
<connect gate="G$1" pin="PC5/ADC15" pad="25"/>
<connect gate="G$1" pin="PC7" pad="38"/>
<connect gate="G$1" pin="PC8" pad="39"/>
<connect gate="G$1" pin="PC9" pad="40"/>
<connect gate="G$1" pin="PD2" pad="54"/>
<connect gate="G$1" pin="PH0/OSC_IN" pad="5"/>
<connect gate="G$1" pin="PH1/OSC_OUT" pad="6"/>
<connect gate="G$1" pin="SPI2_MISO/ADC20/PB14" pad="35"/>
<connect gate="G$1" pin="SPI2_MOSI/ADC21/PB15" pad="36"/>
<connect gate="G$1" pin="SPI2_SCK/ADC19/PB13" pad="34"/>
<connect gate="G$1" pin="UART1_RX/PA10" pad="43"/>
<connect gate="G$1" pin="UART1_TX/PA9" pad="42"/>
<connect gate="G$1" pin="UART3_RX/PC11" pad="52"/>
<connect gate="G$1" pin="UART3_TX/PC10" pad="51"/>
<connect gate="G$1" pin="USB_DM/SPI1_MISO/PA11" pad="44"/>
<connect gate="G$1" pin="USB_DP/SPI1_MOSI/PA12" pad="45"/>
<connect gate="G$1" pin="VDDA" pad="13"/>
<connect gate="G$1" pin="VDD_1" pad="32"/>
<connect gate="G$1" pin="VDD_2" pad="48"/>
<connect gate="G$1" pin="VDD_3" pad="64"/>
<connect gate="G$1" pin="VDD_4" pad="19"/>
<connect gate="G$1" pin="VLCD" pad="1"/>
<connect gate="G$1" pin="VSSA" pad="12"/>
<connect gate="G$1" pin="VSS_1" pad="31"/>
<connect gate="G$1" pin="VSS_2" pad="47"/>
<connect gate="G$1" pin="VSS_3" pad="63"/>
<connect gate="G$1" pin="VSS_4" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F042K-U">
<gates>
<gate name="G$1" symbol="STM32F042K-U"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="G$1" pin="BOOT0-PF11" pad="31"/>
<connect gate="G$1" pin="CAN_RX/I2C1_SCL/USB_DM/PA11" pad="21"/>
<connect gate="G$1" pin="CAN_TX/I2C1_SDA/USB_DP/PA12" pad="22"/>
<connect gate="G$1" pin="GND" pad="EXP"/>
<connect gate="G$1" pin="I2C1_SCL/CAN_RX/PB8" pad="32"/>
<connect gate="G$1" pin="I2C1_SCL/USART1_TX/PB6" pad="29"/>
<connect gate="G$1" pin="I2C1_SDA/USART1_RX/PB7" pad="30"/>
<connect gate="G$1" pin="NRST" pad="4"/>
<connect gate="G$1" pin="PA0/ADC0" pad="6"/>
<connect gate="G$1" pin="PA1/ADC1" pad="7"/>
<connect gate="G$1" pin="PA2/ADC2/USART2_TX" pad="8"/>
<connect gate="G$1" pin="PA3/ADC3/USART2_RX" pad="9"/>
<connect gate="G$1" pin="PA4/ADC4" pad="10"/>
<connect gate="G$1" pin="PA5/ADC5/SPI1_SCK" pad="11"/>
<connect gate="G$1" pin="PA6/ADC6/SPI1_MISO" pad="12"/>
<connect gate="G$1" pin="PA7/ADC7/SPI1_MOSI" pad="13"/>
<connect gate="G$1" pin="PA8" pad="18"/>
<connect gate="G$1" pin="PB0/ADC8" pad="14"/>
<connect gate="G$1" pin="PB1/ADC9" pad="15"/>
<connect gate="G$1" pin="PB2" pad="16"/>
<connect gate="G$1" pin="PF0/I2C1_SDA" pad="2"/>
<connect gate="G$1" pin="PF1/I2C1_SCL" pad="3"/>
<connect gate="G$1" pin="SPI1_MISO/PB4" pad="27"/>
<connect gate="G$1" pin="SPI1_MOSI/PB5" pad="28"/>
<connect gate="G$1" pin="SPI1_SCK/PB3" pad="26"/>
<connect gate="G$1" pin="SWDIO/PA13" pad="23"/>
<connect gate="G$1" pin="USART1_RX/I2C1_SDA/PA10" pad="20"/>
<connect gate="G$1" pin="USART1_TX/I2C1_SCL/PA9" pad="19"/>
<connect gate="G$1" pin="USART2_RX/PA15" pad="25"/>
<connect gate="G$1" pin="USART2_TX/SWCLK/PA14" pad="24"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDDA" pad="5"/>
<connect gate="G$1" pin="VDDIO2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-ARRAY" prefix="CA">
<gates>
<gate name="1" symbol="C"/>
<gate name="2" symbol="C"/>
<gate name="3" symbol="C"/>
<gate name="4" symbol="C"/>
</gates>
<devices>
<device name="" package="1206-ARV-4">
<connects>
<connect gate="1" pin="1" pad="C1A"/>
<connect gate="1" pin="2" pad="C1B"/>
<connect gate="2" pin="1" pad="C2A"/>
<connect gate="2" pin="2" pad="C2B"/>
<connect gate="3" pin="1" pad="C3A"/>
<connect gate="3" pin="2" pad="C3B"/>
<connect gate="4" pin="1" pad="C4A"/>
<connect gate="4" pin="2" pad="C4B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F042K-T" prefix="U">
<gates>
<gate name="G$1" symbol="STM32F042K-T"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="G$1" pin="BOOT0/I2C1_SCL/CAN_RX/PB8" pad="31"/>
<connect gate="G$1" pin="CAN_RX/I2C1_SCL/USB_DM/PA11" pad="21"/>
<connect gate="G$1" pin="CAN_TX/I2C1_SDA/USB_DP/PA12" pad="22"/>
<connect gate="G$1" pin="GND" pad="16 32"/>
<connect gate="G$1" pin="I2C1_SCL/USART1_TX/PB6" pad="29"/>
<connect gate="G$1" pin="I2C1_SDA/USART1_RX/PB7" pad="30"/>
<connect gate="G$1" pin="NRST" pad="4"/>
<connect gate="G$1" pin="PA0/ADC0" pad="6"/>
<connect gate="G$1" pin="PA1/ADC1" pad="7"/>
<connect gate="G$1" pin="PA2/ADC2/USART2_TX" pad="8"/>
<connect gate="G$1" pin="PA3/ADC3/USART2_RX" pad="9"/>
<connect gate="G$1" pin="PA4/ADC4" pad="10"/>
<connect gate="G$1" pin="PA5/ADC5/SPI1_SCK" pad="11"/>
<connect gate="G$1" pin="PA6/ADC6/SPI1_MISO" pad="12"/>
<connect gate="G$1" pin="PA7/ADC7/SPI1_MOSI" pad="13"/>
<connect gate="G$1" pin="PA8" pad="18"/>
<connect gate="G$1" pin="PB0/ADC8" pad="14"/>
<connect gate="G$1" pin="PB1/ADC9" pad="15"/>
<connect gate="G$1" pin="PF0/I2C1_SDA" pad="2"/>
<connect gate="G$1" pin="PF1/I2C1_SCL" pad="3"/>
<connect gate="G$1" pin="SPI1_MISO/PB4" pad="27"/>
<connect gate="G$1" pin="SPI1_MOSI/PB5" pad="28"/>
<connect gate="G$1" pin="SPI1_SCK/PB3" pad="26"/>
<connect gate="G$1" pin="SWDIO/PA13" pad="23"/>
<connect gate="G$1" pin="USART1_RX/I2C1_SDA/PA10" pad="20"/>
<connect gate="G$1" pin="USART1_TX/I2C1_SCL/PA9" pad="19"/>
<connect gate="G$1" pin="USART2_RX/PA15" pad="25"/>
<connect gate="G$1" pin="USART2_TX/SWCLK/PA14" pad="24"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDDA" pad="5"/>
<connect gate="G$1" pin="VDDIO2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F031G6U6" prefix="U">
<gates>
<gate name="G$1" symbol="STM32F031G6U6"/>
</gates>
<devices>
<device name="" package="UFQFPN28">
<connects>
<connect gate="G$1" pin="BOOT0" pad="1"/>
<connect gate="G$1" pin="I2C1_SCL/USART1_TX/PB6" pad="27"/>
<connect gate="G$1" pin="I2C1_SDA/USART1_RX/PB7" pad="28"/>
<connect gate="G$1" pin="NRST" pad="4"/>
<connect gate="G$1" pin="PA0" pad="6"/>
<connect gate="G$1" pin="PA1/TIM2_2" pad="7"/>
<connect gate="G$1" pin="PA2/TIM2_3/USART1_TX" pad="8"/>
<connect gate="G$1" pin="PA3/TIM2_4/USART1_RX" pad="9"/>
<connect gate="G$1" pin="PA4/SPI1_NSS/TIM14_1" pad="10"/>
<connect gate="G$1" pin="PA5/SPI1_SCK" pad="11"/>
<connect gate="G$1" pin="PA6/SPI1_MISO/TIM3_1" pad="12"/>
<connect gate="G$1" pin="PA7/SPI1_MOSI/TIM3_2" pad="13"/>
<connect gate="G$1" pin="PB0/TIM3_3" pad="14"/>
<connect gate="G$1" pin="PB1/TIM3_4" pad="15"/>
<connect gate="G$1" pin="PF0/OSC_IN" pad="2"/>
<connect gate="G$1" pin="PF1/OSC_OUT" pad="3"/>
<connect gate="G$1" pin="SPI1_MISO/TIM3_1/PB4" pad="25"/>
<connect gate="G$1" pin="SPI1_MOSI/TIM3_2/PB5" pad="26"/>
<connect gate="G$1" pin="SPI1_NSS/USART1_RX/PA15" pad="23"/>
<connect gate="G$1" pin="SPI1_SCK/TIM2_2/PB3" pad="24"/>
<connect gate="G$1" pin="SWDIO/PA13" pad="21"/>
<connect gate="G$1" pin="TIM1_1/MCO/PA8" pad="18"/>
<connect gate="G$1" pin="UART1_TX/TIM1_2/I2C1_SCL/PA9" pad="19"/>
<connect gate="G$1" pin="USART1_TX/SWCLK/PA14" pad="22"/>
<connect gate="G$1" pin="USART1_TX/TIM1_3/I2C1_SDA/PA10" pad="20"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VDDA" pad="5"/>
<connect gate="G$1" pin="VSS" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POGOPIN-CONN-4" prefix="J">
<gates>
<gate name="G$1" symbol="POGOPROG-CONN-4"/>
</gates>
<devices>
<device name="" package="POGOPROG-CONN-4-ALLSMT">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SWCLK" pad="3"/>
<connect gate="G$1" pin="SWDIO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VG-4231CE">
<description>TXVCOscillator</description>
<gates>
<gate name="1" symbol="TXVCO"/>
</gates>
<devices>
<device name="" package="CRYSTAL-3.2X2.5">
<connects>
<connect gate="1" pin="CNTRL" pad="1"/>
<connect gate="1" pin="GND" pad="2"/>
<connect gate="1" pin="OUT" pad="3"/>
<connect gate="1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3531-3.3">
<gates>
<gate name="G$1" symbol="LTC3531"/>
</gates>
<devices>
<device name="" package="TSOT23-6">
<connects>
<connect gate="G$1" pin="!SHDN" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW1" pad="6"/>
<connect gate="G$1" pin="SW2" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UPG2214TB">
<description>RF Switch 3GHz - CEL - UPG2214TB-E4-A</description>
<gates>
<gate name="G$1" symbol="UPG2214TB"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="RF_IN" pad="5"/>
<connect gate="G$1" pin="VC1" pad="6"/>
<connect gate="G$1" pin="VC2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA_915MHZ">
<description>Chip Antenna 915MHz - Johanson Technology - 0915AT43A0026E</description>
<gates>
<gate name="G$1" symbol="ANTENNA"/>
</gates>
<devices>
<device name="" package="JOHANSON-TECH_ANTENNA_915MHZ">
<connects>
<connect gate="G$1" pin="ANTENNA" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMIS-201-F">
<gates>
<gate name="G$1" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="LAIRD_BMI-S-101">
<connects>
<connect gate="G$1" pin="SHIELD" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F042C6T6">
<gates>
<gate name="G$1" symbol="STM32F042C6T6"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="NRST" pad="7"/>
<connect gate="G$1" pin="PA0\" pad="10"/>
<connect gate="G$1" pin="PA1" pad="11"/>
<connect gate="G$1" pin="PA10" pad="31"/>
<connect gate="G$1" pin="PA11" pad="32"/>
<connect gate="G$1" pin="PA12" pad="33"/>
<connect gate="G$1" pin="PA13" pad="34"/>
<connect gate="G$1" pin="PA14" pad="37"/>
<connect gate="G$1" pin="PA15" pad="38"/>
<connect gate="G$1" pin="PA2" pad="12"/>
<connect gate="G$1" pin="PA3" pad="13"/>
<connect gate="G$1" pin="PA4" pad="14"/>
<connect gate="G$1" pin="PA5" pad="15"/>
<connect gate="G$1" pin="PA6" pad="16"/>
<connect gate="G$1" pin="PA7" pad="17"/>
<connect gate="G$1" pin="PA8" pad="29"/>
<connect gate="G$1" pin="PA9" pad="30"/>
<connect gate="G$1" pin="PB0" pad="18"/>
<connect gate="G$1" pin="PB1" pad="19"/>
<connect gate="G$1" pin="PB10" pad="21"/>
<connect gate="G$1" pin="PB11" pad="22"/>
<connect gate="G$1" pin="PB12" pad="25"/>
<connect gate="G$1" pin="PB13" pad="26"/>
<connect gate="G$1" pin="PB14" pad="27"/>
<connect gate="G$1" pin="PB15" pad="28"/>
<connect gate="G$1" pin="PB2" pad="20"/>
<connect gate="G$1" pin="PB3" pad="39"/>
<connect gate="G$1" pin="PB4" pad="40"/>
<connect gate="G$1" pin="PB5" pad="41"/>
<connect gate="G$1" pin="PB6" pad="42"/>
<connect gate="G$1" pin="PB7" pad="43"/>
<connect gate="G$1" pin="PB8" pad="45"/>
<connect gate="G$1" pin="PB9" pad="46"/>
<connect gate="G$1" pin="PC13" pad="2"/>
<connect gate="G$1" pin="PC14" pad="3"/>
<connect gate="G$1" pin="PC15" pad="4"/>
<connect gate="G$1" pin="PF0/OSC-IN" pad="5"/>
<connect gate="G$1" pin="PF1/OSC_OUT" pad="6"/>
<connect gate="G$1" pin="PF11/BOOT0" pad="44"/>
<connect gate="G$1" pin="VBAT" pad="1"/>
<connect gate="G$1" pin="VDD1" pad="48"/>
<connect gate="G$1" pin="VDD2" pad="24"/>
<connect gate="G$1" pin="VDDA" pad="9"/>
<connect gate="G$1" pin="VDDAIO" pad="36"/>
<connect gate="G$1" pin="VSS1" pad="35"/>
<connect gate="G$1" pin="VSS2" pad="23"/>
<connect gate="G$1" pin="VSS3" pad="47"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX31865">
<description>&lt;b&gt;RTD to Digital Converter&lt;/b&gt;&lt;br /&gt;&lt;br /&gt;
The MAX31865 is a resistance-to-digital 
converter optimized for platinum resistance temperature 
detectors (RTDs).&lt;br /&gt;&lt;br /&gt;An external resistor sets the sensitivity 
for the RTD being used and a delta-sigma ADC 
converts the ratio of the RTD resistance to the reference 
resistance into digital form. The MAX31865???s inputs are 
protected against overvoltage faults up to +/-50V. 
Programmable detection of RTD and cable open and 
short conditions is included.</description>
<gates>
<gate name="G$1" symbol="MAX31865"/>
</gates>
<devices>
<device name="QFN20" package="QFN20">
<connects>
<connect gate="G$1" pin="!CS" pad="13"/>
<connect gate="G$1" pin="!DRDY" pad="18"/>
<connect gate="G$1" pin="BIAS" pad="1"/>
<connect gate="G$1" pin="DGND" pad="15"/>
<connect gate="G$1" pin="DVDD" pad="19"/>
<connect gate="G$1" pin="FORCE+" pad="5"/>
<connect gate="G$1" pin="FORCE-" pad="9"/>
<connect gate="G$1" pin="FORCE2" pad="6"/>
<connect gate="G$1" pin="GND1" pad="16 P$1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="ISENSOR" pad="4"/>
<connect gate="G$1" pin="REFIN+" pad="2"/>
<connect gate="G$1" pin="REFIN-" pad="3"/>
<connect gate="G$1" pin="RTDIN+" pad="7"/>
<connect gate="G$1" pin="RTDIN-" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="12"/>
<connect gate="G$1" pin="SDI" pad="11"/>
<connect gate="G$1" pin="SDO" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN20-5X5" package="QFN20-5X5">
<connects>
<connect gate="G$1" pin="!CS" pad="13"/>
<connect gate="G$1" pin="!DRDY" pad="18"/>
<connect gate="G$1" pin="BIAS" pad="1"/>
<connect gate="G$1" pin="DGND" pad="15"/>
<connect gate="G$1" pin="DVDD" pad="19"/>
<connect gate="G$1" pin="FORCE+" pad="5"/>
<connect gate="G$1" pin="FORCE-" pad="9"/>
<connect gate="G$1" pin="FORCE2" pad="6"/>
<connect gate="G$1" pin="GND1" pad="16 P$1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="ISENSOR" pad="4"/>
<connect gate="G$1" pin="REFIN+" pad="2"/>
<connect gate="G$1" pin="REFIN-" pad="3"/>
<connect gate="G$1" pin="RTDIN+" pad="7"/>
<connect gate="G$1" pin="RTDIN-" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="12"/>
<connect gate="G$1" pin="SDI" pad="11"/>
<connect gate="G$1" pin="SDO" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POGOPIN-BACKBOARD-SWD">
<gates>
<gate name="G$1" symbol="POGOPROG-CONN-4"/>
</gates>
<devices>
<device name="" package="POGOPROG-BACKMOUNT-SWD">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SWCLK" pad="3"/>
<connect gate="G$1" pin="SWDIO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPV1050" prefix="U">
<gates>
<gate name="G$1" symbol="SPV1050"/>
</gates>
<devices>
<device name="" package="VFQFPN20-3X3">
<connects>
<connect gate="G$1" pin="BATT" pad="14"/>
<connect gate="G$1" pin="BATT_CHG" pad="7"/>
<connect gate="G$1" pin="BATT_CON" pad="8"/>
<connect gate="G$1" pin="CONF" pad="13"/>
<connect gate="G$1" pin="EOC" pad="9"/>
<connect gate="G$1" pin="GND" pad="4 PAD"/>
<connect gate="G$1" pin="IN_HV" pad="20"/>
<connect gate="G$1" pin="IN_LV" pad="16"/>
<connect gate="G$1" pin="LDO1" pad="11"/>
<connect gate="G$1" pin="LDO1_EN" pad="5"/>
<connect gate="G$1" pin="LDO2" pad="12"/>
<connect gate="G$1" pin="LDO2_EN" pad="6"/>
<connect gate="G$1" pin="L_HV" pad="19"/>
<connect gate="G$1" pin="MPP" pad="1"/>
<connect gate="G$1" pin="MPP_REF" pad="3"/>
<connect gate="G$1" pin="MPP_SET" pad="2"/>
<connect gate="G$1" pin="PGND" pad="18"/>
<connect gate="G$1" pin="STORE" pad="15"/>
<connect gate="G$1" pin="UVP" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIREPAD">
<gates>
<gate name="G$1" symbol="WIREPAD"/>
</gates>
<devices>
<device name="" package="WIREPAD">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AAT3681A" prefix="U1">
<description>AAT3681A lipo battery charging ic</description>
<gates>
<gate name="U1" symbol="AAT3681A"/>
</gates>
<devices>
<device name="" package="SC70JW-8">
<connects>
<connect gate="U1" pin="ADP" pad="4"/>
<connect gate="U1" pin="BAT" pad="3"/>
<connect gate="U1" pin="EN" pad="1"/>
<connect gate="U1" pin="GND" pad="6 7 8"/>
<connect gate="U1" pin="ISET" pad="2"/>
<connect gate="U1" pin="STAT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SF1186G" prefix="U1">
<description>SF1186G SAW filter</description>
<gates>
<gate name="U1" symbol="SF1186G"/>
</gates>
<devices>
<device name="" package="SF1186G">
<connects>
<connect gate="U1" pin="GND" pad="2 4"/>
<connect gate="U1" pin="IN" pad="1"/>
<connect gate="U1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AOZ1282CI" prefix="U1">
<description>AOZ1282CI switching regulator</description>
<gates>
<gate name="U1" symbol="AOZ1282CI"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="U1" pin="BS" pad="1"/>
<connect gate="U1" pin="EN" pad="4"/>
<connect gate="U1" pin="FB" pad="3"/>
<connect gate="U1" pin="GND" pad="2"/>
<connect gate="U1" pin="LX" pad="6"/>
<connect gate="U1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN65HVD234" prefix="U1">
<gates>
<gate name="G$1" symbol="SN65HVD234"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="CANH" pad="PIN7"/>
<connect gate="G$1" pin="CANL" pad="PIN6"/>
<connect gate="G$1" pin="D" pad="PIN1"/>
<connect gate="G$1" pin="EN" pad="PIN5"/>
<connect gate="G$1" pin="GND" pad="PIN2"/>
<connect gate="G$1" pin="R" pad="PIN4"/>
<connect gate="G$1" pin="RS" pad="PIN8"/>
<connect gate="G$1" pin="VCC" pad="PIN3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD1CAN" prefix="D">
<description>&lt;b&gt;CAN bus ESD protection diode&lt;/b&gt;&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/PESD1CAN.pdf</description>
<gates>
<gate name="G$1" symbol="PESD1CAN"/>
</gates>
<devices>
<device name="SOT-23" package="SOT23">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT-323" package="SOT323-R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP16301" prefix="U1">
<description>MCP16301 switching regulator</description>
<gates>
<gate name="U1" symbol="MCP16301"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="U1" pin="BOOST" pad="1"/>
<connect gate="U1" pin="EN" pad="4"/>
<connect gate="U1" pin="FB" pad="3"/>
<connect gate="U1" pin="GND" pad="2"/>
<connect gate="U1" pin="SW" pad="6"/>
<connect gate="U1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Y">
<description>TSX-3225 crystal oscillator</description>
<gates>
<gate name="Y1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="TSX-3225">
<connects>
<connect gate="Y1" pin="1" pad="1"/>
<connect gate="Y1" pin="2" pad="3"/>
<connect gate="Y1" pin="3" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ABM8G" package="ABM8G">
<connects>
<connect gate="Y1" pin="1" pad="1"/>
<connect gate="Y1" pin="2" pad="3"/>
<connect gate="Y1" pin="3" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTC" prefix="U">
<description>PTC fuse</description>
<gates>
<gate name="U1" symbol="PTC"/>
</gates>
<devices>
<device name="1206" package="PTC-1206">
<connects>
<connect gate="U1" pin="3" pad="1"/>
<connect gate="U1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BANANA-CONN" prefix="J">
<description>&lt;b&gt;Female PCB Mount Horizontal Banana Jack&lt;/b&gt;
&lt;p&gt;&lt;u&gt; Example Part Numbers&lt;/u&gt;
&lt;br&gt;MAN1: TE Connectivity AMP Connectors
&lt;br&gt;MPN1: 3-582118-0
&lt;br&gt;MAN2: Cinch Connectivity Solutions Johnson
&lt;br&gt;MPN2: 105-0753-001</description>
<gates>
<gate name="G$1" symbol="BANANA-CONN"/>
</gates>
<devices>
<device name="" package="BANANA-PCB-HOR-TH">
<connects>
<connect gate="G$1" pin="1" pad="P$1 P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACS711" prefix="U">
<description>&lt;b&gt;Hall Effect Linear Current Sensor&lt;/b&gt;
&lt;p&gt;&lt;u&gt;Part Number&lt;/u&gt;
&lt;br&gt;MAN: Allegro MicroSystems, LLC
&lt;br&gt;MPN: ACS711KLCTR-25AB-T</description>
<gates>
<gate name="G$1" symbol="ACS7XX"/>
</gates>
<devices>
<device name="" package="SO8">
<connects>
<connect gate="G$1" pin="!FAULT" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IP+" pad="1 2"/>
<connect gate="G$1" pin="IP-" pad="3 4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VIOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVS-BI" prefix="D">
<description>&lt;b&gt;Bi-Directional TVS Diode&lt;/b&gt;
&lt;p&gt;&lt;u&gt;Part Number&lt;/u&gt;
&lt;br&gt;MAN: Bourns Inc.
&lt;br&gt;MPN: SMBJ60CA</description>
<gates>
<gate name="G$1" symbol="DIODE-TVS"/>
</gates>
<devices>
<device name="" package="SMB">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6024" prefix="U">
<description>&lt;b&gt;Hall Effect Linear Current Sensor&lt;/b&gt;
&lt;p&gt;&lt;u&gt;Part Number&lt;/u&gt;
&lt;br&gt;MAN: Microchip Technology
&lt;br&gt;MPN: MCP6024T-I/ST</description>
<gates>
<gate name="A" symbol="OPAMP_2"/>
<gate name="B" symbol="OPAMP_2_1"/>
<gate name="C" symbol="OPAMP_2_1"/>
<gate name="D" symbol="OPAMP_2_1"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN1" pad="3"/>
<connect gate="A" pin="+V" pad="4"/>
<connect gate="A" pin="-IN1" pad="2"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="OUT1" pad="1"/>
<connect gate="B" pin="+IN2" pad="5"/>
<connect gate="B" pin="-IN2" pad="6"/>
<connect gate="B" pin="OUT2" pad="7"/>
<connect gate="C" pin="+IN2" pad="10"/>
<connect gate="C" pin="-IN2" pad="9"/>
<connect gate="C" pin="OUT2" pad="8"/>
<connect gate="D" pin="+IN2" pad="12"/>
<connect gate="D" pin="-IN2" pad="13"/>
<connect gate="D" pin="OUT2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HCPL-181">
<gates>
<gate name="G$1" symbol="OK"/>
</gates>
<devices>
<device name="SOP4" package="SOP4">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="COL" pad="4"/>
<connect gate="G$1" pin="EMIT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
