<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="RJ45-8_SMD-1">
</package>
<package name="0603-ARV-4">
</package>
<package name="RJ45-8_SMD-2">
</package>
<package name="TSSOP16">
</package>
<package name="LED-SMD-10W-DX">
</package>
<package name="LED-SMD-10W-DX-W_POUR">
</package>
<package name="SOT23-5">
</package>
<package name="SRN6045">
</package>
<package name="SUPERMILEAGE-SILK-V1.1">
</package>
<package name="2X3-PINHEADER-SMT">
</package>
<package name="POGOPROG-BACKMOUNT">
</package>
<package name="POGOPROG-CONN">
<description>Standard pogo pin programming header with two alignment holes. Small SMD pads.</description>
</package>
<package name="POGOPROG_LOGO">
</package>
<package name="POGOPROG-CONN-W">
<description>Standard pogo pin programming header with two alignment holes. WIDE smd pads.</description>
</package>
<package name="POGOPROG-CONN-1H">
<description>Standard pogo pin programming header with ONE alignment hole. Small SMD pads.</description>
</package>
<package name="POGOPROG-CONN-0H">
<description>No holes, 2 vias, pogo pin programming header.</description>
</package>
<package name="POGOPROG-CONN-OH-SMALLERVIAS">
<description>No holes, 2 vias, pogo pin programming header. With smaller vias.</description>
</package>
<package name="POGOPROG-CONN-OH-1V">
<description>No holes, 1 via, pogo pin programming header.</description>
</package>
<package name="PROTOFUSION_LOGO_STOP">
</package>
<package name="TREES_STOP">
</package>
<package name="TREES_SNOW_SILK">
</package>
<package name="TREES_SNOW_SM_SILK">
</package>
<package name="RS485-ADAPTER-LOGO-SILK">
</package>
<package name="LED-SMD-10W-DX-STOPONLY">
</package>
<package name="LZ4">
</package>
<package name="LUMA-LOGO-4">
</package>
<package name="ETHANZONCA-SILK">
</package>
<package name="NICKORLANDO-SILK">
</package>
<package name="LUMASITE-SILK">
</package>
<package name="ETHANZONCA-SILK-350DPI">
</package>
<package name="NICKORLANDO-SILK-350DPI">
</package>
<package name="LUMA-SHORT-SILK-350DPI">
</package>
<package name="JULY2013-SILK-350DPI">
</package>
<package name="LUMA-SILK-350DPI">
</package>
<package name="LUMA-SITE-350DPI">
</package>
<package name="MSOP-8_POWERPAD">
</package>
</packages>
<symbols>
<symbol name="RJ45-8">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="GND0"/>
<pin name="GND1"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="STP04CM05XTTR">
<description>Linear LED Driver (UNPROVEN!)</description>
<pin name="VCC"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
<pin name="OUT0"/>
<pin name="NOE"/>
<pin name="GND"/>
<pin name="SDO"/>
<pin name="REXT"/>
</symbol>
<symbol name="LED-RGB">
<pin name="R-" direction="pas"/>
<pin name="R+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="B-" direction="pas"/>
<pin name="B+" direction="pas"/>
</symbol>
<symbol name="AL8805">
<pin name="SW"/>
<pin name="GND"/>
<pin name="CTRL"/>
<pin name="VIN"/>
<pin name="SET"/>
</symbol>
<symbol name="LED">
<pin name="R-" direction="pas"/>
<pin name="R+" direction="pas"/>
</symbol>
<symbol name="L">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="AVR-ISP">
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="\RST"/>
<pin name="VTG"/>
<pin name="MOSI"/>
<pin name="GND"/>
</symbol>
<symbol name="POGOPROG-BACKBOARD">
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="\RST"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="BODY1"/>
<pin name="BODY2"/>
</symbol>
<symbol name="POGOPROG-CONN">
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="\RST"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="LED-LZ4-RGBW">
<pin name="B+"/>
<pin name="B-"/>
<pin name="R+"/>
<pin name="R-"/>
<pin name="G+"/>
<pin name="G-"/>
<pin name="W+"/>
<pin name="W-"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="AUDIO-AMP-MONO-3.1W">
<pin name="SHUTDOWN"/>
<pin name="BYPASS"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="VO+"/>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="VO-"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RJ45">
<description>&lt;b&gt;RJ45 Jack&lt;/b&gt;
Simple RJ45, 8-pin connection - connector for common Cat5, Cat5e, and Cat6 Ethernet cables. 
&lt;br&gt;&lt;br&gt;
MOLEX SMD P/N: 43743-8101</description>
<gates>
<gate name="G$1" symbol="RJ45-8"/>
</gates>
<devices>
<device name="BIGPKG" package="RJ45-8_SMD-1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="GND0" pad="P$9"/>
<connect gate="G$1" pin="GND1" pad="P$10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALLPKG" package="RJ45-8_SMD-2">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="GND0" pad="P$9"/>
<connect gate="G$1" pin="GND1" pad="P$10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-ARRAY">
<gates>
<gate name="A" symbol="RESISTOR"/>
<gate name="B" symbol="RESISTOR"/>
<gate name="C" symbol="RESISTOR"/>
<gate name="D" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="0603-ARV-4">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STP04CM05XTTR">
<description>Linear LED Driver (UNPROVEN!)</description>
<gates>
<gate name="G$1" symbol="STP04CM05XTTR"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="GND" pad="1 2"/>
<connect gate="G$1" pin="LE" pad="5"/>
<connect gate="G$1" pin="NOE" pad="13"/>
<connect gate="G$1" pin="OUT0" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="REXT" pad="15"/>
<connect gate="G$1" pin="SDI" pad="3"/>
<connect gate="G$1" pin="SDO" pad="14"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-10W">
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="PAD" package="LED-SMD-10W-DX">
<connects>
<connect gate="G$1" pin="B+" pad="B+"/>
<connect gate="G$1" pin="B-" pad="B-"/>
<connect gate="G$1" pin="G+" pad="G+"/>
<connect gate="G$1" pin="G-" pad="G-"/>
<connect gate="G$1" pin="R+" pad="R+"/>
<connect gate="G$1" pin="R-" pad="R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AL8805">
<description>DC/DC constant-current buck for driving LEDs (up to 1A)</description>
<gates>
<gate name="G$1" symbol="AL8805"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CTRL" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SET" pad="4"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-10W-MODULAR">
<gates>
<gate name="RED" symbol="LED"/>
<gate name="GREEN" symbol="LED"/>
<gate name="BLUE" symbol="LED"/>
</gates>
<devices>
<device name="WITHCOPPER" package="LED-SMD-10W-DX">
<connects>
<connect gate="BLUE" pin="R+" pad="B+"/>
<connect gate="BLUE" pin="R-" pad="B-"/>
<connect gate="GREEN" pin="R+" pad="G+"/>
<connect gate="GREEN" pin="R-" pad="G-"/>
<connect gate="RED" pin="R+" pad="R+"/>
<connect gate="RED" pin="R-" pad="R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="STOPONLY" package="LED-SMD-10W-DX-STOPONLY">
<connects>
<connect gate="BLUE" pin="R+" pad="B+"/>
<connect gate="BLUE" pin="R-" pad="B-"/>
<connect gate="GREEN" pin="R+" pad="G+"/>
<connect gate="GREEN" pin="R-" pad="G-"/>
<connect gate="RED" pin="R+" pad="R+"/>
<connect gate="RED" pin="R-" pad="R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRN6045">
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="SRN6045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-ISP">
<gates>
<gate name="G$1" symbol="AVR-ISP"/>
</gates>
<devices>
<device name="" package="2X3-PINHEADER-SMT">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VTG" pad="2"/>
<connect gate="G$1" pin="\RST" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POGOPIN-BACKBOARD">
<gates>
<gate name="G$1" symbol="POGOPROG-BACKBOARD"/>
</gates>
<devices>
<device name="" package="POGOPROG-BACKMOUNT">
<connects>
<connect gate="G$1" pin="BODY1" pad="1"/>
<connect gate="G$1" pin="BODY2" pad="8"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MISO" pad="5"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="\RST" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POGOPIN-CONN">
<description>Protofusion custom pogo pin programming header</description>
<gates>
<gate name="J" symbol="POGOPROG-CONN"/>
</gates>
<devices>
<device name="STANDARD" package="POGOPROG-CONN">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS" package="POGOPROG-CONN-0H">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ONEHOLE" package="POGOPROG-CONN-1H">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS-SMV" package="POGOPROG-CONN-OH-SMALLERVIAS">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="POGOPROG-CONN-W">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS-1V" package="POGOPROG-CONN-OH-1V">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZ4-RGBW">
<gates>
<gate name="G$1" symbol="LED-LZ4-RGBW"/>
</gates>
<devices>
<device name="" package="LZ4">
<connects>
<connect gate="G$1" pin="B+" pad="7"/>
<connect gate="G$1" pin="B-" pad="8"/>
<connect gate="G$1" pin="G+" pad="5"/>
<connect gate="G$1" pin="G-" pad="6"/>
<connect gate="G$1" pin="R+" pad="3"/>
<connect gate="G$1" pin="R-" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20 P$21 P$22 P$23 P$24 P$25 P$26 P$27 P$28 P$29 P$30 P$31 P$32 P$33 P$34 P$35 P$36 P$37 P$38 P$39 THERMAL"/>
<connect gate="G$1" pin="W+" pad="1"/>
<connect gate="G$1" pin="W-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZ4-RGBW-FLAT" package="LZ4">
<connects>
<connect gate="G$1" pin="B+" pad="2"/>
<connect gate="G$1" pin="B-" pad="7"/>
<connect gate="G$1" pin="G+" pad="1"/>
<connect gate="G$1" pin="G-" pad="8"/>
<connect gate="G$1" pin="R+" pad="3"/>
<connect gate="G$1" pin="R-" pad="6"/>
<connect gate="G$1" pin="THERMAL" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20 P$21 P$22 P$23 P$24 P$25 P$26 P$27 P$28 P$29 P$30 P$31 P$32 P$33 P$34 P$35 P$36 P$37 P$38 P$39 THERMAL"/>
<connect gate="G$1" pin="W+" pad="4"/>
<connect gate="G$1" pin="W-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO-AMP-MONO-3.1W">
<description>Part No.: TPA6211A1TDGNRQ1</description>
<gates>
<gate name="G$1" symbol="AUDIO-AMP-MONO-3.1W"/>
</gates>
<devices>
<device name="" package="MSOP-8_POWERPAD">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
