<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.28" y2="0" width="0" layer="20"/>
<wire x1="54.28" y1="0" x2="54.28" y2="53.33" width="0" layer="20"/>
<wire x1="54.28" y1="53.33" x2="0" y2="53.33" width="0" layer="20"/>
<wire x1="0" y1="53.33" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICRO-SD-SOCKET-PP">
</package>
<package name="XBEE-SMD">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="0603">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="2X3-NS">
</package>
<package name="TRIMPOT-3MM">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Module">
<packages>
<package name="28P-1.1-22.5X17">
</package>
</packages>
</library>
<library name="jst">
<packages>
<package name="B3B-ZR">
<description>&lt;b&gt;JST ZH Connector&lt;/b&gt;
Top Entry type&lt;br&gt;
3 pol, 1.5 mm Pitch&lt;br&gt;
Source: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eZH.pdf"&gt;http://www.jst-mfg.com/product/pdf/eng/eZH.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="trackuino">
<packages>
<package name="HX1">
</package>
</packages>
</library>
<library name="con-coax">
<packages>
<package name="BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
</packages>
</library>
<library name="74xx-little-us">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="jumper">
<packages>
<package name="05">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="MSOP10">
<description>10-Lead Mini Small Outline Package [MSOP]</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="SparkFun" package="MICRO-SD-SOCKET-PP" value="USD-SOCKETNEW"/>
<element name="U$2" library="SparkFun" package="XBEE-SMD" value="XBEE-1B3"/>
<element name="C1" library="SparkFun" package="0603-CAP" value="18pf"/>
<element name="C2" library="SparkFun" package="0603-CAP" value="18pf"/>
<element name="R1" library="SparkFun" package="0603-RES" value="10k"/>
<element name="IC1" library="atmel" package="TQFP44" value="ATMEGA644P">
<attribute name="OC_NEWARK" value="58M3748"/>
<attribute name="MPN" value="ATMEGA644PV-10AU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1455123"/>
</element>
<element name="Y2" library="SparkFun" package="CRYSTAL-SMD-5X3" value="11.0592MHz"/>
<element name="U1" library="Module" package="28P-1.1-22.5X17" value=""/>
<element name="C6" library="SparkFun" package="0603-CAP" value=""/>
<element name="C7" library="SparkFun" package="0603-CAP" value=""/>
<element name="C8" library="SparkFun" package="0603-CAP" value="8.2pF"/>
<element name="C9" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="C11" library="SparkFun" package="0603-CAP" value=""/>
<element name="C12" library="SparkFun" package="0603-CAP" value=""/>
<element name="C13" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="C14" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="C15" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="C16" library="SparkFun" package="0603-CAP" value="10uF"/>
<element name="C17" library="SparkFun" package="0603-CAP" value="10uF"/>
<element name="L1" library="SparkFun" package="0603" value=""/>
<element name="VBATT" library="jst" package="B3B-ZR" value="B3B-ZR"/>
<element name="BUZZ" library="jst" package="B3B-ZR" value="B3B-ZR"/>
<element name="U3" library="SparkFun" package="SOT223" value="V_REG_317SMD"/>
<element name="J1" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="M2" library="trackuino" package="HX1" value="HX1"/>
<element name="X1" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X2" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="R2" library="SparkFun" package="0603-RES" value="10k"/>
<element name="R3" library="SparkFun" package="0603-RES" value="100k"/>
<element name="IC2" library="74xx-little-us" package="SOT23-5" value="ON M74VHC1GT125DT1G"/>
<element name="J2" library="jumper" package="05" value="J5MM"/>
<element name="L2" library="SparkFun" package="0603" value="10uH"/>
<element name="R4" library="SparkFun" package="0603-RES" value="1k"/>
<element name="R5" library="SparkFun" package="0603-RES" value="2k"/>
<element name="R6" library="SparkFun" package="0603-RES" value="3.9"/>
<element name="R7" library="SparkFun" package="0603-RES" value="8.2"/>
<element name="R8" library="SparkFun" package="0603-RES" value="510k"/>
<element name="R9" library="SparkFun" package="TRIMPOT-3MM" value="30k"/>
<element name="C4" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="TX" library="adafruit" package="CHIPLED_0603" value="GREEN"/>
<element name="STAT" library="adafruit" package="CHIPLED_0603" value="BLUE"/>
<element name="ERROR" library="adafruit" package="CHIPLED_0603" value="RED"/>
<element name="POWER" library="adafruit" package="CHIPLED_0603" value="WHITE"/>
<element name="IC4" library="adafruit" package="MSOP10" value="ISL1209"/>
<element name="R10" library="SparkFun" package="0603-RES" value="100k"/>
<element name="R11" library="SparkFun" package="0603-RES" value="100k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="39"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="6"/>
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="5"/>
<contactref element="M2" pad="0V"/>
<contactref element="M2" pad="RFGND2"/>
<contactref element="M2" pad="RFGND1"/>
<contactref element="X1" pad="2"/>
<contactref element="M2" pad="BODYGND1"/>
<contactref element="M2" pad="BODYGND2"/>
<contactref element="X2" pad="2"/>
<contactref element="X2" pad="4"/>
<contactref element="X2" pad="3"/>
<contactref element="X2" pad="5"/>
<contactref element="J1" pad="6"/>
<contactref element="U$2" pad="10"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U$2" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="TX" pad="C"/>
<contactref element="STAT" pad="C"/>
<contactref element="ERROR" pad="C"/>
<contactref element="POWER" pad="C"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="7"/>
<contactref element="Y2" pad="3"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="8"/>
<contactref element="Y2" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="20"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="TCK">
<contactref element="IC1" pad="21"/>
</signal>
<signal name="TMS">
<contactref element="IC1" pad="22"/>
</signal>
<signal name="TDO">
<contactref element="IC1" pad="23"/>
</signal>
<signal name="TDI">
<contactref element="IC1" pad="24"/>
</signal>
<signal name="RXD0">
<contactref element="IC1" pad="9"/>
</signal>
<signal name="TXD0">
<contactref element="IC1" pad="10"/>
</signal>
<signal name="RXD1">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="TXD1">
<contactref element="IC1" pad="12"/>
</signal>
<signal name="+5V">
<contactref element="IC2" pad="5"/>
</signal>
<signal name="RFOUT">
<contactref element="M2" pad="RFOUT"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="HX1_EN">
<contactref element="IC2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="IC1" pad="36"/>
<contactref element="TX" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="2"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="17"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="38"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="HX1_EN_5V">
<contactref element="M2" pad="EN"/>
<contactref element="IC2" pad="4"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="29"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="3.3_RXD0">
<contactref element="U$2" pad="2"/>
</signal>
<signal name="3.3_TXD0">
<contactref element="U$2" pad="3"/>
</signal>
<signal name="SOMEANALOGPIN">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="VBATT" pad="2"/>
</signal>
<signal name="5V">
<contactref element="M2" pad="VCC"/>
</signal>
<signal name="HX1_TXD_5V">
<contactref element="M2" pad="TXD"/>
</signal>
<signal name="N$5">
<contactref element="L2" pad="1"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="35"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="34"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="33"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="32"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="SINBEFORE">
<contactref element="R7" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="HX1_TX_3.3">
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R9" pad="3"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="IC4" pad="3"/>
</signal>
<signal name="VDD">
<contactref element="IC4" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
