<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="61.9" y2="0" width="0" layer="20"/>
<wire x1="61.9" y1="0" x2="61.9" y2="39.36" width="0" layer="20"/>
<wire x1="61.9" y1="39.36" x2="0" y2="39.36" width="0" layer="20"/>
<wire x1="0" y1="39.36" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XBEE-SMD">
</package>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="0805">
</package>
<package name="SRU1038">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="1X10_LOCK">
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="0603">
</package>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SeniorDesign">
<packages>
<package name="SOIC8HEAT">
</package>
<package name="CD08RM0SB">
</package>
<package name="SOT23-5">
</package>
</packages>
</library>
<library name="SLAT-CON-JST-ZH">
<packages>
<package name="ZH-H-2-1">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun" package="XBEE-SMD" value="XBEE-1B3"/>
<element name="IC1" library="atmel" package="TQFP44" value="ATMEGA644A">
<attribute name="OC_NEWARK" value="58M3748"/>
<attribute name="MPN" value="ATMEGA644PV-10AU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1455123"/>
</element>
<element name="R1" library="SparkFun" package="0603-RES" value="10k"/>
<element name="C1" library="SparkFun" package="0603-CAP" value=""/>
<element name="C2" library="SparkFun" package="0603-CAP" value=""/>
<element name="C3" library="SparkFun" package="0603-CAP" value=""/>
<element name="C4" library="SparkFun" package="0603-CAP" value="8.2pF"/>
<element name="C5" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="C6" library="SparkFun" package="0603-CAP" value=""/>
<element name="C7" library="SparkFun" package="0603-CAP" value=""/>
<element name="3.3V_SWITCHING" library="SeniorDesign" package="SOIC8HEAT" value="IFX91041EJ V33"/>
<element name="BATT" library="SLAT-CON-JST-ZH" package="ZH-H-2-1" value="ZH-H-2-1"/>
<element name="Q6" library="transistor-small-signal" package="SOT23" value="BSH202"/>
<element name="C8" library="SparkFun" package="0805" value="100uF"/>
<element name="C9" library="SparkFun" package="0603-CAP" value="22nF"/>
<element name="R2" library="SparkFun" package="0603-RES" value="22k"/>
<element name="C10" library="SparkFun" package="0603-CAP" value="220nF"/>
<element name="L3" library="SparkFun" package="SRU1038" value="47uH"/>
<element name="D1" library="SparkFun" package="SMA-DIODE" value="DIODE-SCHOTTKY"/>
<element name="C11" library="SparkFun" package="0603-CAP" value="220nF"/>
<element name="C12" library="SparkFun" package="0805" value="100uF"/>
<element name="ROTARY_DIP" library="SeniorDesign" package="CD08RM0SB" value="CD08RM0SB"/>
<element name="TEMP" library="SeniorDesign" package="SOT23-5" value="MCP9800"/>
<element name="JP2" library="SparkFun" package="1X10_LOCK" value="M10LOCK"/>
<element name="JP1" library="SparkFun" package="1X10_LOCK" value="M10LOCK"/>
<element name="R3" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="R4" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="R5" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="C13" library="SparkFun" package="0603-CAP" value="18pf"/>
<element name="C14" library="SparkFun" package="0603-CAP" value="18pf"/>
<element name="Y2" library="SparkFun" package="CRYSTAL-SMD-5X3" value="11.0592MHz"/>
<element name="C15" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="L2" library="SparkFun" package="0603" value="10uH"/>
<element name="C16" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="C17" library="SparkFun" package="0603-CAP" value=".1uF"/>
<element name="C18" library="SparkFun" package="0603-CAP" value="10uF"/>
<element name="ICSP" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="R6" library="SparkFun" package="0603-RES" value="4.7k"/>
<element name="R7" library="SparkFun" package="0603-RES" value="4.7k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="10"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="39"/>
<contactref element="3.3V_SWITCHING" pad="2"/>
<contactref element="3.3V_SWITCHING" pad="9"/>
<contactref element="C8" pad="2"/>
<contactref element="3.3V_SWITCHING" pad="1"/>
<contactref element="BATT" pad="2"/>
<contactref element="Q6" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="39"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="ICSP" pad="6"/>
<contactref element="TEMP" pad="2"/>
<contactref element="U$1" pad="10"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="ROTARY_DIP" pad="C2"/>
<contactref element="ROTARY_DIP" pad="C1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="AVCC">
<contactref element="IC1" pad="27"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="38"/>
<contactref element="IC1" pad="17"/>
<contactref element="IC1" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="3.3V_SWITCHING" pad="4"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="L2" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="TEMP" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="ICSP" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="BATT" pad="1"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="VBAT">
<contactref element="Q6" pad="2"/>
<contactref element="3.3V_SWITCHING" pad="8"/>
<contactref element="3.3V_SWITCHING" pad="7"/>
<contactref element="C8" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="3.3V_SWITCHING" pad="3"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="3.3V_SWITCHING" pad="5"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="3.3V_SWITCHING" pad="6"/>
<contactref element="C10" pad="2"/>
<contactref element="L3" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="20"/>
<contactref element="TEMP" pad="5"/>
<contactref element="R7" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="19"/>
<contactref element="TEMP" pad="4"/>
<contactref element="R6" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="PA0">
<contactref element="IC1" pad="37"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="PA1">
<contactref element="IC1" pad="36"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="PA2">
<contactref element="IC1" pad="35"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="PA3">
<contactref element="IC1" pad="34"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="PA4">
<contactref element="IC1" pad="33"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="PA5">
<contactref element="IC1" pad="32"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="PA6">
<contactref element="IC1" pad="31"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="PA7">
<contactref element="IC1" pad="30"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="3"/>
<contactref element="ICSP" pad="3"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="2"/>
<contactref element="ICSP" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="1"/>
<contactref element="ICSP" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="Y2" pad="3"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="Y2" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="L2" pad="1"/>
</signal>
<signal name="RXD0">
<contactref element="IC1" pad="9"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="TXD0">
<contactref element="IC1" pad="10"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="RXD1">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="TXD1">
<contactref element="IC1" pad="12"/>
</signal>
<signal name="PD7">
<contactref element="IC1" pad="16"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="PD6">
<contactref element="IC1" pad="15"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="PD5">
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="PD4">
<contactref element="IC1" pad="13"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="DIP1">
<contactref element="ROTARY_DIP" pad="2"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="DIP3">
<contactref element="ROTARY_DIP" pad="8"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="DIP2">
<contactref element="ROTARY_DIP" pad="4"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="DIP0">
<contactref element="ROTARY_DIP" pad="1"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="PWM0">
<contactref element="IC1" pad="40"/>
</signal>
<signal name="PWM1">
<contactref element="IC1" pad="41"/>
</signal>
<signal name="PWM2">
<contactref element="IC1" pad="42"/>
</signal>
<signal name="PWM3">
<contactref element="IC1" pad="43"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
