<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="34.29" x2="0" y2="5.08" width="0" layer="20"/>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="0" x2="30.48" y2="0" width="0" layer="20"/>
<wire x1="30.48" y1="0" x2="35.56" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="35.56" y1="5.08" x2="35.56" y2="34.29" width="0" layer="20"/>
<wire x1="35.56" y1="34.29" x2="30.48" y2="39.37" width="0" layer="20" curve="90"/>
<wire x1="30.48" y1="39.37" x2="5.08" y2="39.37" width="0" layer="20"/>
<wire x1="5.08" y1="39.37" x2="0" y2="34.29" width="0" layer="20" curve="90"/>
<text>DO NOT MOVE RINGS, PIN HEADERS, OR PCB DIMMENSIONS. THEY ARE ACCURATELY PLACED</text>
<text>Miter edges to radius of .2</text>
<text>.</text>
<text>.</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10_LOCK">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SLAT-CON-JST-ZH">
<packages>
<package name="ZH-H-2-1">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SeniorDesign">
<packages>
<package name="CU_LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X10_LOCK" value="M10LOCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X10_LOCK" value="M10LOCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SLAT-CON-JST-ZH" package="ZH-H-2-1" value="ZH-H-2-1"/>
<element name="J2" library="SLAT-CON-JST-ZH" package="ZH-H-2-1" value="ZH-H-2-1"/>
<element name="J3" library="SLAT-CON-JST-ZH" package="ZH-H-2-1" value="ZH-H-2-1"/>
<element name="LED1" library="adafruit" package="CHIPLED_0603" value="GREEN"/>
<element name="R1" library="SparkFun" package="0603-RES" value="65"/>
<element name="LED2" library="adafruit" package="CHIPLED_0603" value="BLUE"/>
<element name="R2" library="SparkFun" package="0603-RES" value="65"/>
<element name="LED3" library="adafruit" package="CHIPLED_0603" value="RED"/>
<element name="R3" library="SparkFun" package="0603-RES" value="65"/>
<element name="U$1" library="SeniorDesign" package="CU_LOGO" value="CU_LOGO"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="VBAT">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="6"/>
</signal>
<signal name="PD4">
<contactref element="JP1" pad="7"/>
</signal>
<signal name="PD5">
<contactref element="JP1" pad="8"/>
</signal>
<signal name="PD6">
<contactref element="JP1" pad="9"/>
</signal>
<signal name="PD7">
<contactref element="JP1" pad="10"/>
</signal>
<signal name="SCL">
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="JP2" pad="2"/>
</signal>
<signal name="PA0">
<contactref element="JP2" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PA1">
<contactref element="JP2" pad="4"/>
<contactref element="J2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="PA2">
<contactref element="JP2" pad="5"/>
<contactref element="J3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="PA3">
<contactref element="JP2" pad="6"/>
</signal>
<signal name="PA4">
<contactref element="JP2" pad="7"/>
</signal>
<signal name="PA5">
<contactref element="JP2" pad="8"/>
</signal>
<signal name="PA6">
<contactref element="JP2" pad="9"/>
</signal>
<signal name="PA7">
<contactref element="JP2" pad="10"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="LED3" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$5">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$19">
</signal>
</signals>
</board>
</drawing>
</eagle>
