<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="2.286" y1="0" x2="86.614" y2="0" width="0" layer="20"/>
<wire x1="86.614" y1="0" x2="88.9" y2="2.286" width="0" layer="20" curve="90"/>
<wire x1="88.9" y1="2.286" x2="88.9" y2="42.164" width="0" layer="20"/>
<wire x1="88.9" y1="42.164" x2="86.614" y2="44.45" width="0" layer="20" curve="90"/>
<wire x1="86.614" y1="44.45" x2="2.286" y2="44.45" width="0" layer="20"/>
<wire x1="2.286" y1="44.45" x2="0" y2="42.164" width="0" layer="20" curve="90"/>
<wire x1="0" y1="42.164" x2="0" y2="2.286" width="0" layer="20"/>
<wire x1="0" y1="2.286" x2="2.286" y2="0" width="0" layer="20" curve="90"/>
<hole x="85.725" y="41.275" drill="3.2"/>
<hole x="85.725" y="3.175" drill="3.2"/>
<hole x="3.175" y="41.275" drill="3.2"/>
<hole x="3.175" y="3.175" drill="3.2"/>
<text>VIN</text>
<text>VIN</text>
<text>CANH</text>
<text>CANL</text>
<text>CANL</text>
<text>CANH</text>
<text>GND</text>
<text>GND</text>
<text>Status</text>
<text>Error</text>
<text>CAN</text>
<text>OUTPUT8</text>
<text>OUTPUT7</text>
<text>OUTPUT6</text>
<text>OUTPUT5</text>
<text>- +</text>
<text>INPUT1</text>
<text>INPUT2</text>
<text>INPUT3</text>
<text>INPUT4</text>
<text>OUT1</text>
<text>OUT2</text>
<text>OUT3</text>
<text>OUT4</text>
<text>OUT5</text>
<text>OUT6</text>
<text>OUT7</text>
<text>OUT8</text>
<text>IN1</text>
<text>IN2</text>
<text>IN3</text>
<text>IN4</text>
<text>IN5</text>
<text>IN6</text>
<text>IN7</text>
<text>IN8</text>
<text>OUTPUT4</text>
<text>OUTPUT3</text>
<text>OUTPUT2</text>
<text>OUTPUT1</text>
<text>- +</text>
<text>- +</text>
<text>- +</text>
<text>- +</text>
<text>- +</text>
<text>- +</text>
<text>- +</text>
<text>INPUT5</text>
<text>INPUT6</text>
<text>INPUT7</text>
<text>INPUT8</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
<text>GND</text>
<text>V+</text>
<text>SIG</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="NRG4026">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
<package name="SOT23-3@1">
</package>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="Protofusion">
<packages>
<package name="LQFP32">
</package>
<package name="SOIC8">
<description>SOIC8 package type.</description>
</package>
<package name="SOT23-6">
</package>
<package name="POGOPROG-CONN-4-ALLSMT">
</package>
<package name="ABM8G">
</package>
<package name="MICROFET_2X2">
<description>&lt;b&gt;1206-8 ChipFET&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/72593/72593.pdf&lt;br&gt;
http://www.vishay.com/docs/71151/71151.pdf</description>
</package>
<package name="PTC-1206">
</package>
<package name="JST-PA-4">
</package>
<package name="JST-PA-2">
</package>
<package name="JST-PA-3">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="Protofusion-logos">
<packages>
<package name="HYDROBOT-LOGO">
</package>
<package name="BYPROTOFUSION-LOGO">
</package>
<package name="RELAYDRIVE">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MINI-FLAT-16">
<description>&lt;b&gt;TOSHIBA PHOTOCOUPLER GaAs IRED &amp; PHOTO-TRANSISTOR&lt;/b&gt; 11-10F1&lt;/b&gt;&lt;p&gt;
Source: http://www.semicon.toshiba.co.jp/td/en/Opto/Photocoupler/en_20050928_TLP283_datasheet.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Protofusion-logos" package="HYDROBOT-LOGO" value=""/>
<element name="U$3" library="Protofusion-logos" package="BYPROTOFUSION-LOGO" value=""/>
<element name="R202" library="SparkFun-Resistors" package="0402-RES" value="31.6K 1%"/>
<element name="R203" library="SparkFun-Resistors" package="0402-RES" value="10K 1%"/>
<element name="L201" library="SparkFun-Passives" package="NRG4026" value="15uH"/>
<element name="C206" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="C205" library="SparkFun-Passives" package="0805" value="4.7uF"/>
<element name="C207" library="SparkFun-Passives" package="0805" value="10uF"/>
<element name="D202" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="D204" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="D205" library="SparkFun-LED" package="LED-0603" value="Blue"/>
<element name="D206" library="SparkFun-LED" package="LED-0603" value="Red"/>
<element name="R204" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="R205" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R206" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="C210" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="U203" library="Protofusion" package="SOIC8" value="SN65HVD234"/>
<element name="U201" library="Protofusion" package="SOT23-6" value="MCP16301"/>
<element name="D203" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="C208" library="SparkFun-Passives" package="0805" value="10uF"/>
<element name="Q201" library="SparkFun-DiscreteSemi" package="SOT23-3@1" value="">
<attribute name="PROD_ID" value="TRANS-08285"/>
</element>
<element name="R201" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D201" library="SparkFun-DiscreteSemi" package="SOD-323" value="8V">
<attribute name="PROD_ID" value="DIO-12442"/>
</element>
<element name="Q101" library="Protofusion" package="MICROFET_2X2" value="N-FET">
<attribute name="PROD_ID" value="TRANS-09516"/>
</element>
<element name="R117" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R121" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D101" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="R118" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R122" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D102" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="R125" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R129" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D105" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="R126" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R130" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D106" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="J111" library="Protofusion" package="POGOPROG-CONN-4-ALLSMT" value="POGOPIN-CONN-4"/>
<element name="U202" library="Protofusion" package="LQFP32" value="STM32F042K-T"/>
<element name="C201" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="C203" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="C209" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="Y201" library="Protofusion" package="ABM8G" value="12MHz"/>
<element name="C204" library="SparkFun-Passives" package="0402-CAP" value="9pF"/>
<element name="C202" library="SparkFun-Passives" package="0402-CAP" value="9pF"/>
<element name="U102" library="optocoupler" package="MINI-FLAT-16" value="TLP283-4">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R101" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R105" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C101" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="U101" library="Protofusion" package="PTC-1206" value="PTC1206"/>
<element name="R102" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R106" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C102" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="R109" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R113" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C105" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="R110" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R114" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C106" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="Q103" library="Protofusion" package="MICROFET_2X2" value="N-FET">
<attribute name="PROD_ID" value="TRANS-09516"/>
</element>
<element name="U$2" library="Protofusion-logos" package="RELAYDRIVE" value=""/>
<element name="U$4" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="D207" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R207" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D208" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R208" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D209" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R209" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D210" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R210" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D211" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R211" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D212" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R212" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D213" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R213" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D214" library="SparkFun-LED" package="LED-0603" value="Yellow"/>
<element name="R214" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="J109" library="Protofusion" package="JST-PA-4" value="JST-PA-4PTH"/>
<element name="J110" library="Protofusion" package="JST-PA-4" value="JST-PA-4PTH"/>
<element name="FRAME101" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LEDGER"/>
<element name="U103" library="optocoupler" package="MINI-FLAT-16" value="TLP283-4">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R103" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R107" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C103" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="R104" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R108" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C104" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="R111" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R115" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C107" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="R112" library="SparkFun-Resistors" package="0402-RES" value="600"/>
<element name="R116" library="SparkFun-Resistors" package="0402-RES" value="10K"/>
<element name="C108" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="Q102" library="Protofusion" package="MICROFET_2X2" value="N-FET">
<attribute name="PROD_ID" value="TRANS-09516"/>
</element>
<element name="R119" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R123" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D103" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="R120" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R124" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D104" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="R127" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R131" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D107" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="R128" library="SparkFun-Resistors" package="0402-RES" value="10"/>
<element name="R132" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="D108" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-11623"/>
</element>
<element name="Q104" library="Protofusion" package="MICROFET_2X2" value="N-FET">
<attribute name="PROD_ID" value="TRANS-09516"/>
</element>
<element name="J112" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J113" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J116" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J117" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J114" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J115" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J118" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J119" library="Protofusion" package="JST-PA-2" value="JST-PA-2PTH"/>
<element name="J101" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="J102" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="J105" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="J106" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="J103" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="J104" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="J107" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="J108" library="Protofusion" package="JST-PA-3" value="JST-PA-3PTH"/>
<element name="D215" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R215" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D216" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R216" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D217" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R217" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D218" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R218" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D219" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R219" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D220" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R220" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D221" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R221" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="D222" library="SparkFun-LED" package="LED-0603" value="Green"/>
<element name="R222" library="SparkFun-Resistors" package="0402-RES" value="200"/>
<element name="Q202" library="SparkFun-DiscreteSemi" package="SOT23-3" value="5.8A/30V/35mΩ">
<attribute name="PROD_ID" value="TRANS-12988"/>
</element>
<element name="R223" library="SparkFun-Resistors" package="0402-RES" value="100K"/>
<element name="FRAME201" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LEDGER"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="U203" pad="PIN3"/>
<contactref element="C210" pad="1"/>
<contactref element="U203" pad="PIN5"/>
<contactref element="L201" pad="2"/>
<contactref element="D203" pad="A"/>
<contactref element="C208" pad="1"/>
<contactref element="C207" pad="2"/>
<contactref element="R202" pad="2"/>
<contactref element="J111" pad="1"/>
<contactref element="U202" pad="1"/>
<contactref element="U202" pad="5"/>
<contactref element="C209" pad="1"/>
<contactref element="U202" pad="17"/>
<contactref element="U102" pad="16"/>
<contactref element="U102" pad="14"/>
<contactref element="U102" pad="12"/>
<contactref element="U102" pad="10"/>
<contactref element="C201" pad="2"/>
<contactref element="C203" pad="2"/>
<contactref element="U103" pad="16"/>
<contactref element="U103" pad="14"/>
<contactref element="U103" pad="12"/>
<contactref element="U103" pad="10"/>
</signal>
<signal name="GND">
<contactref element="U203" pad="PIN2"/>
<contactref element="C210" pad="2"/>
<contactref element="D204" pad="C"/>
<contactref element="D205" pad="C"/>
<contactref element="D206" pad="C"/>
<contactref element="U203" pad="PIN8"/>
<contactref element="C205" pad="2"/>
<contactref element="U201" pad="2"/>
<contactref element="R201" pad="1"/>
<contactref element="D202" pad="A"/>
<contactref element="R203" pad="2"/>
<contactref element="C207" pad="1"/>
<contactref element="C208" pad="2"/>
<contactref element="Q101" pad="S1"/>
<contactref element="R121" pad="1"/>
<contactref element="R122" pad="1"/>
<contactref element="R129" pad="1"/>
<contactref element="R130" pad="1"/>
<contactref element="J111" pad="2"/>
<contactref element="U202" pad="16"/>
<contactref element="U202" pad="32"/>
<contactref element="C209" pad="2"/>
<contactref element="C202" pad="1"/>
<contactref element="C204" pad="2"/>
<contactref element="Y201" pad="2"/>
<contactref element="Y201" pad="4"/>
<contactref element="U102" pad="2"/>
<contactref element="R105" pad="2"/>
<contactref element="C101" pad="2"/>
<contactref element="R106" pad="2"/>
<contactref element="C102" pad="2"/>
<contactref element="U102" pad="4"/>
<contactref element="R113" pad="2"/>
<contactref element="C105" pad="2"/>
<contactref element="U102" pad="6"/>
<contactref element="R114" pad="2"/>
<contactref element="C106" pad="2"/>
<contactref element="U102" pad="8"/>
<contactref element="C201" pad="1"/>
<contactref element="C203" pad="1"/>
<contactref element="Q101" pad="S2"/>
<contactref element="Q103" pad="S1"/>
<contactref element="Q103" pad="S2"/>
<contactref element="J109" pad="4"/>
<contactref element="J110" pad="4"/>
<contactref element="U103" pad="2"/>
<contactref element="R107" pad="2"/>
<contactref element="C103" pad="2"/>
<contactref element="U103" pad="4"/>
<contactref element="R108" pad="2"/>
<contactref element="C104" pad="2"/>
<contactref element="U103" pad="6"/>
<contactref element="R115" pad="2"/>
<contactref element="C107" pad="2"/>
<contactref element="U103" pad="8"/>
<contactref element="R116" pad="2"/>
<contactref element="C108" pad="2"/>
<contactref element="Q102" pad="S1"/>
<contactref element="R123" pad="1"/>
<contactref element="R124" pad="1"/>
<contactref element="Q102" pad="S2"/>
<contactref element="R131" pad="1"/>
<contactref element="Q104" pad="S1"/>
<contactref element="R132" pad="1"/>
<contactref element="Q104" pad="S2"/>
<contactref element="J101" pad="1"/>
<contactref element="J102" pad="1"/>
<contactref element="J105" pad="1"/>
<contactref element="J106" pad="1"/>
<contactref element="J103" pad="1"/>
<contactref element="J104" pad="1"/>
<contactref element="J107" pad="1"/>
<contactref element="J108" pad="1"/>
<contactref element="Q202" pad="2"/>
<contactref element="R223" pad="1"/>
</signal>
<signal name="CAN_H">
<contactref element="U203" pad="PIN7"/>
<contactref element="J109" pad="2"/>
<contactref element="J110" pad="2"/>
</signal>
<signal name="CAN_L">
<contactref element="U203" pad="PIN6"/>
<contactref element="J109" pad="3"/>
<contactref element="J110" pad="3"/>
</signal>
<signal name="LED1">
<contactref element="R204" pad="1"/>
<contactref element="U202" pad="20"/>
</signal>
<signal name="LED2">
<contactref element="R205" pad="1"/>
<contactref element="U202" pad="19"/>
</signal>
<signal name="LED3">
<contactref element="R206" pad="1"/>
<contactref element="U202" pad="18"/>
</signal>
<signal name="CAN_TX">
<contactref element="U203" pad="PIN1"/>
<contactref element="U202" pad="22"/>
</signal>
<signal name="CAN_RX">
<contactref element="U203" pad="PIN4"/>
<contactref element="U202" pad="21"/>
</signal>
<signal name="OSC_IN">
<contactref element="U202" pad="2"/>
<contactref element="Y201" pad="1"/>
<contactref element="C202" pad="2"/>
</signal>
<signal name="OSC_OUT">
<contactref element="U202" pad="3"/>
<contactref element="Y201" pad="3"/>
<contactref element="C204" pad="1"/>
</signal>
<signal name="SWCLK">
<contactref element="J111" pad="3"/>
<contactref element="U202" pad="24"/>
</signal>
<signal name="SWDIO">
<contactref element="J111" pad="4"/>
<contactref element="U202" pad="23"/>
</signal>
<signal name="VIN">
<contactref element="Q201" pad="3"/>
<contactref element="D101" pad="C"/>
<contactref element="D102" pad="C"/>
<contactref element="D105" pad="C"/>
<contactref element="D106" pad="C"/>
<contactref element="J109" pad="1"/>
<contactref element="J110" pad="1"/>
<contactref element="D103" pad="C"/>
<contactref element="D104" pad="C"/>
<contactref element="D107" pad="C"/>
<contactref element="D108" pad="C"/>
<contactref element="J112" pad="1"/>
<contactref element="J113" pad="1"/>
<contactref element="J116" pad="1"/>
<contactref element="J117" pad="1"/>
<contactref element="J114" pad="1"/>
<contactref element="J115" pad="1"/>
<contactref element="J118" pad="1"/>
<contactref element="J119" pad="1"/>
</signal>
<signal name="OUTPUT1">
<contactref element="R117" pad="1"/>
<contactref element="R207" pad="1"/>
<contactref element="U202" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="R202" pad="1"/>
<contactref element="R203" pad="1"/>
<contactref element="U201" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="L201" pad="1"/>
<contactref element="C206" pad="2"/>
<contactref element="D202" pad="C"/>
<contactref element="U201" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="C206" pad="1"/>
<contactref element="U201" pad="1"/>
<contactref element="D203" pad="C"/>
</signal>
<signal name="N$21">
<contactref element="D204" pad="A"/>
<contactref element="R204" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R205" pad="2"/>
<contactref element="D205" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="R206" pad="2"/>
<contactref element="D206" pad="A"/>
</signal>
<signal name="N$25">
<contactref element="R201" pad="2"/>
<contactref element="Q201" pad="1"/>
<contactref element="D201" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="Q101" pad="G1"/>
<contactref element="R117" pad="2"/>
<contactref element="R121" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Q101" pad="D1_2"/>
<contactref element="D101" pad="A"/>
<contactref element="Q101" pad="D1"/>
<contactref element="J112" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R118" pad="2"/>
<contactref element="R122" pad="2"/>
<contactref element="Q101" pad="G2"/>
</signal>
<signal name="N$5">
<contactref element="D102" pad="A"/>
<contactref element="Q101" pad="D2_2"/>
<contactref element="Q101" pad="D2"/>
<contactref element="J113" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R125" pad="2"/>
<contactref element="R129" pad="2"/>
<contactref element="Q103" pad="G1"/>
</signal>
<signal name="N$12">
<contactref element="D105" pad="A"/>
<contactref element="Q103" pad="D1_2"/>
<contactref element="Q103" pad="D1"/>
<contactref element="J116" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R126" pad="2"/>
<contactref element="R130" pad="2"/>
<contactref element="Q103" pad="G2"/>
</signal>
<signal name="N$16">
<contactref element="D106" pad="A"/>
<contactref element="Q103" pad="D2_2"/>
<contactref element="Q103" pad="D2"/>
<contactref element="J117" pad="2"/>
</signal>
<signal name="OUTPUT2">
<contactref element="R118" pad="1"/>
<contactref element="R208" pad="1"/>
<contactref element="U202" pad="7"/>
</signal>
<signal name="OUTPUT3">
<contactref element="R125" pad="1"/>
<contactref element="R209" pad="1"/>
<contactref element="U202" pad="8"/>
</signal>
<signal name="OUTPUT4">
<contactref element="R126" pad="1"/>
<contactref element="R210" pad="1"/>
<contactref element="U202" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="R101" pad="1"/>
<contactref element="J101" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R101" pad="2"/>
<contactref element="U102" pad="1"/>
</signal>
<signal name="INPUT1">
<contactref element="U102" pad="15"/>
<contactref element="R105" pad="1"/>
<contactref element="C101" pad="1"/>
<contactref element="R215" pad="1"/>
<contactref element="U202" pad="11"/>
</signal>
<signal name="N$15">
<contactref element="R102" pad="1"/>
<contactref element="J102" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="R102" pad="2"/>
<contactref element="U102" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="R109" pad="1"/>
<contactref element="J105" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R109" pad="2"/>
<contactref element="U102" pad="5"/>
</signal>
<signal name="N$30">
<contactref element="R110" pad="1"/>
<contactref element="J106" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="R110" pad="2"/>
<contactref element="U102" pad="7"/>
</signal>
<signal name="INPUT2">
<contactref element="R106" pad="1"/>
<contactref element="C102" pad="1"/>
<contactref element="U102" pad="13"/>
<contactref element="R216" pad="1"/>
<contactref element="U202" pad="25"/>
</signal>
<signal name="INPUT4">
<contactref element="R114" pad="1"/>
<contactref element="C106" pad="1"/>
<contactref element="U102" pad="9"/>
<contactref element="R218" pad="1"/>
<contactref element="U202" pad="27"/>
</signal>
<signal name="INPUT3">
<contactref element="R113" pad="1"/>
<contactref element="C105" pad="1"/>
<contactref element="U102" pad="11"/>
<contactref element="R217" pad="1"/>
<contactref element="U202" pad="26"/>
</signal>
<signal name="VCCIO">
<contactref element="U101" pad="1"/>
<contactref element="J101" pad="3"/>
<contactref element="J102" pad="3"/>
<contactref element="J105" pad="3"/>
<contactref element="J106" pad="3"/>
<contactref element="J103" pad="3"/>
<contactref element="J104" pad="3"/>
<contactref element="J107" pad="3"/>
<contactref element="J108" pad="3"/>
</signal>
<signal name="INPUT5">
<contactref element="U103" pad="15"/>
<contactref element="R107" pad="1"/>
<contactref element="C103" pad="1"/>
<contactref element="R219" pad="1"/>
<contactref element="U202" pad="28"/>
</signal>
<signal name="INPUT6">
<contactref element="R108" pad="1"/>
<contactref element="C104" pad="1"/>
<contactref element="U103" pad="13"/>
<contactref element="R220" pad="1"/>
<contactref element="U202" pad="29"/>
</signal>
<signal name="INPUT7">
<contactref element="R115" pad="1"/>
<contactref element="C107" pad="1"/>
<contactref element="U103" pad="11"/>
<contactref element="R221" pad="1"/>
<contactref element="U202" pad="30"/>
</signal>
<signal name="INPUT8">
<contactref element="R116" pad="1"/>
<contactref element="C108" pad="1"/>
<contactref element="U103" pad="9"/>
<contactref element="R222" pad="1"/>
<contactref element="U202" pad="31"/>
</signal>
<signal name="OUTPUT5">
<contactref element="R211" pad="1"/>
<contactref element="R119" pad="1"/>
<contactref element="U202" pad="12"/>
</signal>
<signal name="OUTPUT6">
<contactref element="R212" pad="1"/>
<contactref element="R120" pad="1"/>
<contactref element="U202" pad="13"/>
</signal>
<signal name="OUTPUT7">
<contactref element="R213" pad="1"/>
<contactref element="R127" pad="1"/>
<contactref element="U202" pad="14"/>
</signal>
<signal name="OUTPUT8">
<contactref element="R214" pad="1"/>
<contactref element="R128" pad="1"/>
<contactref element="U202" pad="15"/>
</signal>
<signal name="N$4">
<contactref element="D207" pad="A"/>
<contactref element="R207" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="D208" pad="A"/>
<contactref element="R208" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D209" pad="A"/>
<contactref element="R209" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="D210" pad="A"/>
<contactref element="R210" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="D211" pad="A"/>
<contactref element="R211" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="D212" pad="A"/>
<contactref element="R212" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="D213" pad="A"/>
<contactref element="R213" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="D214" pad="A"/>
<contactref element="R214" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R103" pad="1"/>
<contactref element="J103" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="R103" pad="2"/>
<contactref element="U103" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="R104" pad="1"/>
<contactref element="J104" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="R104" pad="2"/>
<contactref element="U103" pad="3"/>
</signal>
<signal name="N$37">
<contactref element="R111" pad="1"/>
<contactref element="J107" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="R111" pad="2"/>
<contactref element="U103" pad="5"/>
</signal>
<signal name="N$39">
<contactref element="R112" pad="1"/>
<contactref element="J108" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="R112" pad="2"/>
<contactref element="U103" pad="7"/>
</signal>
<signal name="N$41">
<contactref element="Q102" pad="G1"/>
<contactref element="R119" pad="2"/>
<contactref element="R123" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="Q102" pad="D1_2"/>
<contactref element="D103" pad="A"/>
<contactref element="Q102" pad="D1"/>
<contactref element="J114" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="R120" pad="2"/>
<contactref element="R124" pad="2"/>
<contactref element="Q102" pad="G2"/>
</signal>
<signal name="N$44">
<contactref element="D104" pad="A"/>
<contactref element="Q102" pad="D2_2"/>
<contactref element="Q102" pad="D2"/>
<contactref element="J115" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="R127" pad="2"/>
<contactref element="R131" pad="2"/>
<contactref element="Q104" pad="G1"/>
</signal>
<signal name="N$46">
<contactref element="D107" pad="A"/>
<contactref element="Q104" pad="D1_2"/>
<contactref element="Q104" pad="D1"/>
<contactref element="J118" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="R128" pad="2"/>
<contactref element="R132" pad="2"/>
<contactref element="Q104" pad="G2"/>
</signal>
<signal name="N$48">
<contactref element="D108" pad="A"/>
<contactref element="Q104" pad="D2_2"/>
<contactref element="Q104" pad="D2"/>
<contactref element="J119" pad="2"/>
</signal>
<signal name="LED_DIM">
<contactref element="D209" pad="C"/>
<contactref element="D208" pad="C"/>
<contactref element="D211" pad="C"/>
<contactref element="D210" pad="C"/>
<contactref element="D212" pad="C"/>
<contactref element="D213" pad="C"/>
<contactref element="D207" pad="C"/>
<contactref element="D214" pad="C"/>
<contactref element="D217" pad="C"/>
<contactref element="D216" pad="C"/>
<contactref element="D219" pad="C"/>
<contactref element="D218" pad="C"/>
<contactref element="D220" pad="C"/>
<contactref element="D221" pad="C"/>
<contactref element="D215" pad="C"/>
<contactref element="D222" pad="C"/>
<contactref element="Q202" pad="3"/>
</signal>
<signal name="N$49">
<contactref element="D215" pad="A"/>
<contactref element="R215" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="D216" pad="A"/>
<contactref element="R216" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="D217" pad="A"/>
<contactref element="R217" pad="2"/>
</signal>
<signal name="N$52">
<contactref element="D218" pad="A"/>
<contactref element="R218" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="D219" pad="A"/>
<contactref element="R219" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="D220" pad="A"/>
<contactref element="R220" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="D221" pad="A"/>
<contactref element="R221" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="D222" pad="A"/>
<contactref element="R222" pad="2"/>
</signal>
<signal name="LED_DIM_SWITCH">
<contactref element="Q202" pad="1"/>
<contactref element="R223" pad="2"/>
<contactref element="U202" pad="10"/>
</signal>
<signal name="N$57">
</signal>
<signal name="VIN_RECTIFIED">
<contactref element="C205" pad="1"/>
<contactref element="U201" pad="5"/>
<contactref element="U201" pad="4"/>
<contactref element="Q201" pad="2"/>
<contactref element="D201" pad="C"/>
<contactref element="U101" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
