<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="45.085" x2="0.635" y2="4.28625" width="0" layer="20"/>
<wire x1="-2.54" y1="-0.79375" x2="19.05" y2="-0.79375" width="0" layer="20"/>
<wire x1="15.875" y1="4.28625" x2="15.875" y2="45.085" width="0" layer="20"/>
<wire x1="-2.54" y1="50.165" x2="19.05" y2="50.165" width="0" layer="20"/>
<wire x1="19.05" y1="50.165" x2="21.59" y2="47.625" width="0" layer="20" curve="-90"/>
<wire x1="21.59" y1="47.625" x2="19.05" y2="45.085" width="0" layer="20" curve="-90"/>
<wire x1="19.05" y1="45.085" x2="15.875" y2="45.085" width="0" layer="20"/>
<text>CANH</text>
<text>CANL</text>
<text>GND</text>
<text>TERM</text>
<text>Boot</text>
<text>canable.io</text>
<text>CANH</text>
<text>CANL</text>
<text>GND</text>
<text>Pwr</text>
<text>Act</text>
<text>openlight labs</text>
<hole x="19.05" y="47.625" drill="3.175"/>
<wire x1="0.635" y1="45.085" x2="-2.54" y2="45.085" width="0" layer="20"/>
<wire x1="-2.54" y1="45.085" x2="-5.08" y2="47.625" width="0" layer="20" curve="-90"/>
<wire x1="-5.08" y1="47.625" x2="-2.54" y2="50.165" width="0" layer="20" curve="-90"/>
<hole x="-2.54" y="47.625" drill="3.175"/>
<hole x="0.635" y="3.96875" drill="0.381"/>
<hole x="0.635" y="3.33375" drill="0.381"/>
<hole x="0.635" y="2.69875" drill="0.381"/>
<hole x="0.635" y="2.06375" drill="0.381"/>
<hole x="0.635" y="0.79375" drill="0.381"/>
<hole x="0.635" y="1.42875" drill="0.381"/>
<hole x="0.635" y="0.15875" drill="0.381"/>
<text>TERM</text>
<hole x="0.635" y="-0.47625" drill="0.381"/>
<hole x="15.875" y="3.96875" drill="0.381"/>
<hole x="15.875" y="3.33375" drill="0.381"/>
<hole x="15.875" y="2.69875" drill="0.381"/>
<hole x="15.875" y="2.06375" drill="0.381"/>
<hole x="15.875" y="0.79375" drill="0.381"/>
<hole x="15.875" y="1.42875" drill="0.381"/>
<hole x="15.875" y="0.15875" drill="0.381"/>
<hole x="15.875" y="-0.47625" drill="0.381"/>
<hole x="15.875" y="49.8475" drill="0.381"/>
<hole x="15.875" y="49.2125" drill="0.381"/>
<hole x="15.875" y="48.5775" drill="0.381"/>
<hole x="15.875" y="47.9425" drill="0.381"/>
<hole x="15.875" y="46.6725" drill="0.381"/>
<hole x="15.875" y="47.3075" drill="0.381"/>
<hole x="15.875" y="46.0375" drill="0.381"/>
<hole x="15.875" y="45.4025" drill="0.381"/>
<hole x="0.635" y="49.8475" drill="0.381"/>
<hole x="0.635" y="49.2125" drill="0.381"/>
<hole x="0.635" y="48.5775" drill="0.381"/>
<hole x="0.635" y="47.9425" drill="0.381"/>
<hole x="0.635" y="46.6725" drill="0.381"/>
<hole x="0.635" y="47.3075" drill="0.381"/>
<hole x="0.635" y="46.0375" drill="0.381"/>
<hole x="0.635" y="45.4025" drill="0.381"/>
<wire x1="15.875" y1="4.28625" x2="19.05" y2="4.28625" width="0" layer="20"/>
<wire x1="19.05" y1="4.28625" x2="21.59" y2="1.74625" width="0" layer="20" curve="-90"/>
<wire x1="21.59" y1="1.74625" x2="19.05" y2="-0.79375" width="0" layer="20" curve="-90"/>
<hole x="19.05" y="1.74625" drill="3.175"/>
<wire x1="-2.54" y1="4.28625" x2="0.635" y2="4.28625" width="0" layer="20"/>
<wire x1="-2.54" y1="-0.79375" x2="-5.08" y2="1.74625" width="0" layer="20" curve="-90"/>
<wire x1="-5.08" y1="1.74625" x2="-2.54" y2="4.28625" width="0" layer="20" curve="-90"/>
<hole x="-2.54" y="1.74625" drill="3.175"/>
<text>x4</text>
<text>x4</text>
<text>canable</text>
<text>pro 1.1</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK@1">
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -3 Pin PTH Locking&lt;/h3&gt;
Holes are offset 0.007" from center to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Protofusion">
<packages>
<package name="LQFP48">
</package>
<package name="POGOPROG-CONN-4-ALLSMT">
</package>
<package name="SO20W">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="PTC0805">
<description>0805 fuse</description>
</package>
</packages>
</library>
<library name="SLAT-RCL">
<description>SLAT Resisters, Capacitors, Inductors</description>
<packages>
<package name="0603-GEN">
<description>A generic 0603 pad size, similar to 0603-RES and 0603-CAP, but without the silkscreen below the component.</description>
</package>
</packages>
</library>
<library name="SLAT-MISC">
<description>SLAT Miscellaneous</description>
<packages>
<package name="B3U-1000P">
</package>
</packages>
</library>
<library name="SLAT-Diodes">
<description>SLAT Diodes</description>
<packages>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
</packages>
</library>
<library name="Protofusion-passives">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="MF_Connectors">
<packages>
<package name="MICROUSB-RIGHT">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for Micro USB Type B connector. Based on FCI 10118193-0001LF.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="Protofusion-logos">
<packages>
<package name="CANABLE-PRO-1.1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="SparkFun-PowerIC" package="SOT23-5" value="MF-REG-SOT235-3.3V-300mA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="VREG-00822"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="150060BS75000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Protofusion-passives" package="0603-CAP" value="MF-CAP-0603-1uF">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C7" library="Protofusion-passives" package="0603-CAP" value="MF-CAP-0603-1uF">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="R1" library="Protofusion-passives" package="0603-RES" value="MF-RES-0603-560">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Protofusion-passives" package="0603-CAP" value="MF-CAP-0603-0.1uF">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C1" library="Protofusion-passives" package="0603-CAP" value="MF-CAP-0603-0.1uF">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U1" library="Protofusion" package="LQFP48" value="STM32F042C6T6">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
</element>
<element name="J1" library="Protofusion" package="POGOPROG-CONN-4-ALLSMT" value="POGOPIN-CONN-4">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value="MF-LED-0603-GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Protofusion-passives" package="0603-RES" value="MF-RES-0603-560">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Protofusion-passives" package="0603-RES" value="120">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Protofusion-passives" package="0603-CAP" value="MF-CAP-0603-0.1uF">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C6" library="Protofusion-passives" package="0603-CAP" value="MF-CAP-0603-0.1uF">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="R4" library="Protofusion-passives" package="0603-RES" value="MF-RES-0603-10K">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X03_LOCK@1" value="M20-9990346">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="dp_devices" package="PTC0805" value="0ZCK0035FF2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SLAT-RCL" package="0603-GEN" value="MF-RES-0603-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SLAT-RCL" package="0603-GEN" value="MF-CAP-0603-0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SLAT-RCL" package="0603-GEN" value="MF-CAP-0603-0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SLAT-RCL" package="0603-GEN" value="MF-CAP-0603-0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SLAT-RCL" package="0603-GEN" value="0.22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SLAT-RCL" package="0603-GEN" value="MF-CAP-0603-0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SLAT-RCL" package="0603-GEN" value="MF-CAP-0603-0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="SLAT-RCL" package="0603-GEN" value="BLM18KG102SH1D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB2" library="SLAT-RCL" package="0603-GEN" value="BLM18KG102SH1D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-3_LOCK.007S" value="0393570003">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08288"/>
<attribute name="SF_ID" value="PRT-08235"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="SLAT-MISC" package="B3U-1000P" value="B3U-1000P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SLAT-Diodes" package="SOT23-6" value="USBLC6-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="PESD1CAN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="1206" value="MF-CAP-1206-10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-10057"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="1206" value="MF-CAP-1206-10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-10057"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="MF_Connectors" package="MICROUSB-RIGHT" value="MF-CON-MICROUSB-RIGHT">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-CON-MICROUSB-RIGHT"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-MICROUSB-RIGHT"/>
<attribute name="VALUE" value="MF-CON-MICROUSB-RIGHT"/>
</element>
<element name="U5" library="Protofusion" package="SO20W" value="ADM3055E">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="Protofusion-logos" package="CANABLE-PRO-1.1" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="47"/>
<contactref element="LED2" pad="C"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="J3" pad="5"/>
<contactref element="J3" pad="S4"/>
<contactref element="J3" pad="S6"/>
<contactref element="J3" pad="S2"/>
<contactref element="J3" pad="S1"/>
<contactref element="J3" pad="S3"/>
<contactref element="J3" pad="S5"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="U5" pad="10"/>
<contactref element="U5" pad="9"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="5"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="36"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="48"/>
<contactref element="J1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="V_BATT">
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="F1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C12" pad="1"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="D+">
<contactref element="U1" pad="33"/>
<contactref element="J3" pad="3"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="D-">
<contactref element="U1" pad="32"/>
<contactref element="J3" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="LED_RX">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="LED_TX">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="CAN_RX">
<contactref element="U1" pad="45"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="CAN_TX">
<contactref element="U1" pad="46"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="SWDIO">
<contactref element="U1" pad="34"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SWCLK">
<contactref element="U1" pad="37"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="CANH">
<contactref element="R3" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="U5" pad="14"/>
</signal>
<signal name="CANL">
<contactref element="J5" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="BOOT0">
<contactref element="U1" pad="44"/>
<contactref element="R4" pad="2"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$107">
<contactref element="R5" pad="1"/>
<contactref element="U5" pad="12"/>
</signal>
<signal name="N$109">
<contactref element="C11" pad="1"/>
<contactref element="FB2" pad="1"/>
<contactref element="U5" pad="19"/>
</signal>
<signal name="GND_B">
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="FB1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="D1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="C16" pad="2"/>
<contactref element="U5" pad="15"/>
<contactref element="U5" pad="11"/>
</signal>
<signal name="N$110">
<contactref element="C11" pad="2"/>
<contactref element="FB1" pad="1"/>
<contactref element="U5" pad="18"/>
<contactref element="U5" pad="20"/>
</signal>
<signal name="N$111">
<contactref element="FB2" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U5" pad="16"/>
</signal>
<signal name="N$1">
<contactref element="J3" pad="1"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
