<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>Zonca 2023</text>
<wire x1="38.1" y1="40.005" x2="79.375" y2="40.005" width="0.0762" layer="20"/>
<wire x1="79.375" y1="40.005" x2="80.645" y2="38.735" width="0.0762" layer="20" curve="-90"/>
<wire x1="80.645" y1="38.735" x2="80.645" y2="20.701" width="0.0762" layer="20"/>
<wire x1="80.645" y1="20.701" x2="79.375" y2="19.431" width="0.0762" layer="20" curve="-90"/>
<wire x1="36.83" y1="38.735" x2="36.83" y2="20.701" width="0.0762" layer="20"/>
<wire x1="36.83" y1="20.701" x2="38.1" y2="19.431" width="0.0762" layer="20" curve="90"/>
<wire x1="38.1" y1="19.431" x2="79.375" y2="19.431" width="0.0762" layer="20"/>
<wire x1="38.1" y1="40.005" x2="36.83" y2="38.735" width="0.0762" layer="20" curve="90"/>
<text>Tempo CAN</text>
<text>WP r01</text>
<text>openlightlabs.com</text>
<text>Err</text>
<text>Act</text>
<text>CANH</text>
<text>CANL</text>
<text>GND</text>
<text>VIN</text>
<text>MotionCAN r01</text>
<hole x="65.151" y="21.336" drill="2.54"/>
<hole x="38.735" y="38.1" drill="2.54"/>
<hole x="38.735" y="21.336" drill="2.54"/>
<hole x="58.42" y="29.845" drill="2.54"/>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="Protofusion">
<packages>
<package name="POGOPROG-CONN-4-ALLSMT">
</package>
<package name="LQFP48">
</package>
<package name="TSX-3225">
<description>Footprint for TSX-3225 Crystal</description>
</package>
<package name="SOT23-6">
</package>
<package name="SOT23-5">
</package>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="Protofusion-passives">
<packages>
<package name="0805-CAP">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="NRG4026">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="SLAT-MISC">
<description>SLAT Miscellaneous</description>
<packages>
<package name="B3U-1000P">
</package>
</packages>
</library>
<library name="Protofusion-discrete">
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
<package name="SOD-323">
<description>SOD-323 (Small Outline Diode)</description>
</package>
</packages>
</library>
<library name="43045-0400">
<description>&lt;Micro-Fit 3.0 Right-Angle Header, 3.00mm Pitch, Dual Row, 4 Circuits, with Snap-in Plastic Peg PCB Lock&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="43045-04(00,01,02,10)">
<description>&lt;b&gt;43045-04(00,01,02,10)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MF_Connectors">
<packages>
<package name="MICROUSB-RIGHT">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for Micro USB Type B connector. Based on FCI 10118193-0001LF.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="M20-7860346">
<description>&lt;2.54mm (0.1") Pitch SIL SMT Dual Entry Socket Assembly, tin, 3 contacts&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="M207860346">
<description>&lt;b&gt;M20-7860346-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="M20-7910442R">
<description>&lt;2.54mm (0.1") Pitch SIL Horizontal SMT Socket Assembly, selective gold + tin (Tape &amp; Reel packing), 4 contacts&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="M207910442R">
<description>&lt;b&gt;M20-7910442R-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
</packages>
</library>
<library name="44764-0401">
<description>&lt;Headers &amp; Wire Housings R.A. RECPT 4P tin w/friction pegs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="447640401">
<description>&lt;b&gt;44764-0401&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Protofusion-passives" package="0603-RES" value="100">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Protofusion" package="POGOPROG-CONN-4-ALLSMT" value="POGOPIN-CONN-4">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="SparkFun-DigitalIC" package="SO08" value="SN65HVD232DR">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09907"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="SLAT-MISC" package="B3U-1000P" value="B3U-1000P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="Protofusion" package="LQFP48" value="STM32F042C6T6 STM32F302">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
</element>
<element name="C28" library="Protofusion-passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="Protofusion-passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="Protofusion-passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="Protofusion-passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="Protofusion-passives" package="0603-RES" value="100k">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="Protofusion" package="TSX-3225" value="CRYSTAL">
<attribute name="DIGIKEY_PART_NUMBER" value="SER4180CT-ND"/>
<attribute name="MANUFACTURER" value="EPSON"/>
<attribute name="PART_NUMBER" value="TSX-3225 24.0000MF15X-AC6"/>
</element>
<element name="C9" library="Protofusion-passives" package="0603-CAP" value="9pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="Protofusion-passives" package="0603-CAP" value="9pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Protofusion-discrete" package="SOT23-3" value="PFET">
<attribute name="DIGIKEY_PART_NUMBER" value="1727-PMV100EPARCT-ND"/>
<attribute name="MANUFACTURER" value="Nexperia USA Inc."/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="PMV100EPAR"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="Protofusion-passives" package="0603-RES" value="100K">
<attribute name="DIGIKEY_PART_NUMBER" value="P100KJCT-ND"/>
<attribute name="MANUFACTURER" value="Panasonic Electronic Components"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="ERJ-2GEJ104X"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="Protofusion-discrete" package="SOD-323" value="12V">
<attribute name="DIGIKEY_PART_NUMBER" value="MM3Z12VST1GOSCT-ND"/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="MM3Z12VST1G"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Protofusion-discrete" package="SOD-323" value="28V">
<attribute name="DIGIKEY_PART_NUMBER" value="DF2B36FUH3FCT-ND"/>
<attribute name="MANUFACTURER" value="Toshiba Semiconductor and Storage"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="DF2B36FU,H3F"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="Protofusion" package="SOT23-6" value="AP63205WU-7">
<attribute name="DIGIKEY_PART_NUMBER" value="AP63205WU-7DICT-ND"/>
<attribute name="MANUFACTURER" value="Diodes Incorporated"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="AP63205WU-7"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Protofusion-passives" package="NRG4026" value="4.7uH NRS4018T4R7MDGJ">
<attribute name="DIGIKEY_PART_NUMBER" value="587-2893-2-ND"/>
<attribute name="MANUFACTURER" value="Taiyo Yuden"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="NRS4018T4R7MDGJ"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="Protofusion-passives" package="0805-CAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="Protofusion-passives" package="0805-CAP" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="Protofusion-passives" package="0805-CAP" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="Protofusion-passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Protofusion-passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-0603" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="Protofusion-passives" package="0603-RES" value="100">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-0603" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="Protofusion-passives" package="0603-RES" value="100">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="43045-0400" package="43045-04(00,01,02,10)" value="43045-0400">
<attribute name="DESCRIPTION" value="Micro-Fit 3.0 Right-Angle Header, 3.00mm Pitch, Dual Row, 4 Circuits, with Snap-in Plastic Peg PCB Lock"/>
<attribute name="HEIGHT" value="9.9mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="43045-0400"/>
<attribute name="MOUSER_PART_NUMBER" value="538-43045-0400"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/43045-0400?qs=UeCeOHRHQeaIqmxE9Bxdrw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="MF_Connectors" package="MICROUSB-RIGHT" value="MF-CON-MICROUSB-RIGHT">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-CON-MICROUSB-RIGHT"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-MICROUSB-RIGHT"/>
</element>
<element name="J3" library="M20-7860346" package="M207860346" value="M20-7860346">
<attribute name="DESCRIPTION" value="2.54mm (0.1&quot;) Pitch SIL SMT Dual Entry Socket Assembly, tin, 3 contacts"/>
<attribute name="HEIGHT" value="7.5mm"/>
<attribute name="MANUFACTURER_NAME" value="Harwin"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="M20-7860346"/>
<attribute name="MOUSER_PART_NUMBER" value="855-M20-7860346"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Harwin/M20-7860346?qs=l5IOXVh7iow%252BtpnOWExuzg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="M20-7910442R" package="M207910442R" value="M20-7910442R">
<attribute name="DESCRIPTION" value="2.54mm (0.1&quot;) Pitch SIL Horizontal SMT Socket Assembly, selective gold + tin (Tape &amp; Reel packing), 4 contacts"/>
<attribute name="HEIGHT" value="2.65mm"/>
<attribute name="MANUFACTURER_NAME" value="Harwin"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="M20-7910442R"/>
<attribute name="MOUSER_PART_NUMBER" value="855-M20-7910442R"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Harwin/M20-7910442R?qs=k41KVqW3ymrGT4VqB8J8Xw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Protofusion" package="SOT23-5" value="MIC5501">
<attribute name="DIGIKEY_PART_NUMBER" value="576-4879-1-ND"/>
<attribute name="MANUFACTURER" value="Microchip Technology"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="MIC5504-1.8YM5-TR"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Protofusion-passives" package="0805-CAP" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Protofusion-passives" package="0603-RES" value="49.9K">
<attribute name="DIGIKEY_PART_NUMBER" value="P100KJCT-ND"/>
<attribute name="MANUFACTURER" value="Panasonic Electronic Components"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="ERJ-2GEJ104X"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Protofusion-passives" package="0603-RES" value="100K">
<attribute name="DIGIKEY_PART_NUMBER" value="P100KJCT-ND"/>
<attribute name="MANUFACTURER" value="Panasonic Electronic Components"/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value="ERJ-2GEJ104X"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="microbuilder" package="SOD-323" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="Protofusion" package="SOT23" value="PESD1CANSOT-23">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="NAME"/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="44764-0401" package="447640401" value="44764-0401">
<attribute name="DESCRIPTION" value="Headers &amp; Wire Housings R.A. RECPT 4P tin w/friction pegs"/>
<attribute name="HEIGHT" value="10.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="44764-0401"/>
<attribute name="MOUSER_PART_NUMBER" value="538-44764-0401"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/44764-0401?qs=hPE3sep%2FRHa1aBWMNcba1Q%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="LED1" pad="C"/>
<contactref element="J1" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="U8" pad="8"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="U9" pad="8"/>
<contactref element="U9" pad="35"/>
<contactref element="U9" pad="23"/>
<contactref element="U9" pad="47"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="Y1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="R17" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U7" pad="4"/>
<contactref element="C32" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="J3" pad="3"/>
<contactref element="J6" pad="5"/>
<contactref element="J6" pad="S1"/>
<contactref element="J6" pad="S3"/>
<contactref element="J6" pad="S4"/>
<contactref element="J6" pad="S5"/>
<contactref element="J6" pad="S2"/>
<contactref element="J6" pad="S6"/>
<contactref element="R3" pad="1"/>
<contactref element="D6" pad="3"/>
<contactref element="J4" pad="1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="J1" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="U9" pad="48"/>
<contactref element="U9" pad="24"/>
<contactref element="U9" pad="9"/>
<contactref element="C31" pad="1"/>
<contactref element="U9" pad="36"/>
<contactref element="U9" pad="1"/>
<contactref element="U8" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="D+">
<contactref element="U9" pad="33"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="D-">
<contactref element="U9" pad="32"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="LED_PWR">
<contactref element="R1" pad="1"/>
<contactref element="U9" pad="25"/>
</signal>
<signal name="SWCLK">
<contactref element="J1" pad="3"/>
<contactref element="U9" pad="37"/>
</signal>
<signal name="SWDIO">
<contactref element="J1" pad="4"/>
<contactref element="U9" pad="34"/>
</signal>
<signal name="CAN_RX">
<contactref element="U8" pad="4"/>
<contactref element="U9" pad="45"/>
</signal>
<signal name="CAN_TX">
<contactref element="U8" pad="1"/>
<contactref element="U9" pad="46"/>
</signal>
<signal name="CANH">
<contactref element="U8" pad="7"/>
<contactref element="D6" pad="1"/>
<contactref element="J4" pad="4"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="CANL">
<contactref element="U8" pad="6"/>
<contactref element="J4" pad="3"/>
<contactref element="D6" pad="2"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="BOOT0">
<contactref element="SW1" pad="1"/>
<contactref element="U9" pad="44"/>
<contactref element="R16" pad="1"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="Y1" pad="1"/>
<contactref element="U9" pad="5"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U9" pad="6"/>
<contactref element="Y1" pad="3"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="J7" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R17" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="U7" pad="3"/>
<contactref element="C16" pad="2"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U7" pad="5"/>
<contactref element="L1" pad="1"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U7" pad="6"/>
<contactref element="C36" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="D3" pad="A"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="D4" pad="A"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="LED_STAT">
<contactref element="R18" pad="1"/>
<contactref element="U9" pad="42"/>
</signal>
<signal name="LED_ERR">
<contactref element="R19" pad="1"/>
<contactref element="U9" pad="41"/>
</signal>
<signal name="PIR_OUT">
<contactref element="J3" pad="1"/>
<contactref element="U9" pad="11"/>
</signal>
<signal name="5V">
<contactref element="U7" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="J5" pad="1"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="TRIG">
<contactref element="J5" pad="2"/>
<contactref element="U9" pad="12"/>
</signal>
<signal name="ECHO">
<contactref element="J5" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="ECHO_DIV">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="U9" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="J6" pad="1"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
