<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<packages>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="0402-RES">
</package>
<package name="0402-CAP">
</package>
<package name="0805-CAP">
</package>
<package name="0805-RES">
</package>
<package name="0402-INDUCTOR">
</package>
<package name="0603-INDUCTOR">
</package>
<package name="0805-INDUCTOR">
</package>
<package name="1206-ARV-4">
</package>
<package name="0603-ARV-4">
</package>
<package name="SRN6045">
</package>
<package name="NRG4026">
</package>
<package name="MAL219691204E3">
</package>
<package name="LPS4012">
</package>
<package name="1008-INDUCTOR">
<description>1008 inductor footprint</description>
</package>
<package name="1206-CAP">
</package>
</packages>
<symbols>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP-POLAR">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>Chip resistor</description>
<gates>
<gate name="R1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="0402" package="0402-RES">
<connects>
<connect gate="R1" pin="1" pad="1"/>
<connect gate="R1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
<device name="0603" package="0603-RES">
<connects>
<connect gate="R1" pin="1" pad="1"/>
<connect gate="R1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
<device name="0805" package="0805-RES">
<connects>
<connect gate="R1" pin="1" pad="1"/>
<connect gate="R1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR" prefix="C" uservalue="yes">
<description>Ceramic capacitor</description>
<gates>
<gate name="C1" symbol="CAP"/>
</gates>
<devices>
<device name="0402" package="0402-CAP">
<connects>
<connect gate="C1" pin="1" pad="1"/>
<connect gate="C1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="0603" package="0603-CAP">
<connects>
<connect gate="C1" pin="1" pad="1"/>
<connect gate="C1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="0805" package="0805-CAP">
<connects>
<connect gate="C1" pin="1" pad="1"/>
<connect gate="C1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="1206" package="1206-CAP">
<connects>
<connect gate="C1" pin="1" pad="1"/>
<connect gate="C1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>Inductor</description>
<gates>
<gate name="L1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="0402" package="0402-INDUCTOR">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
<device name="0603" package="0603-INDUCTOR">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
<device name="0805" package="0805-INDUCTOR">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
<device name="SRN6045" package="SRN6045">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value="SRN6045-100MCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc."/>
<attribute name="PART_NUMBER" value="SRN6045-100M"/>
<attribute name="TOLERANCE" value="20%"/>
</technology>
</technologies>
</device>
<device name="NRG4026" package="NRG4026">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
<device name="LPS4012" package="LPS4012">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value="Coilcraft"/>
<attribute name="PART_NUMBER" value="LPS4012-103MRB"/>
</technology>
</technologies>
</device>
<device name="1008" package="1008-INDUCTOR">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-ARRAY" prefix="CA" uservalue="yes">
<description>Surface mount capacitor array</description>
<gates>
<gate name="A" symbol="CAP"/>
<gate name="B" symbol="CAP"/>
<gate name="C" symbol="CAP"/>
<gate name="D" symbol="CAP"/>
</gates>
<devices>
<device name="1206" package="1206-ARV-4">
<connects>
<connect gate="A" pin="1" pad="A1"/>
<connect gate="A" pin="2" pad="A2"/>
<connect gate="B" pin="1" pad="B1"/>
<connect gate="B" pin="2" pad="B2"/>
<connect gate="C" pin="1" pad="C1"/>
<connect gate="C" pin="2" pad="C2"/>
<connect gate="D" pin="1" pad="D1"/>
<connect gate="D" pin="2" pad="D2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-ARRAY" prefix="RA" uservalue="yes">
<description>Surface mount resistor array</description>
<gates>
<gate name="A" symbol="RESISTOR"/>
<gate name="B" symbol="RESISTOR"/>
<gate name="C" symbol="RESISTOR"/>
<gate name="D" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="0603-ARV-4">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY_PART_NUMBER" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
<attribute name="TOLERANCE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-POLAR" prefix="C" uservalue="yes">
<gates>
<gate name="C?" symbol="CAP-POLAR"/>
</gates>
<devices>
<device name="" package="MAL219691204E3">
<connects>
<connect gate="C?" pin="+" pad="1"/>
<connect gate="C?" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER" value=""/>
<attribute name="PART_NUMBER" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
