<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="33.02" y1="19.030875" x2="33.02" y2="-1.254175" width="0" layer="20"/>
<wire x1="33.02" y1="-1.254175" x2="30.464175" y2="-3.81" width="0" layer="20" curve="-90"/>
<wire x1="30.464175" y1="-3.81" x2="27.94" y2="-1.285825" width="0" layer="20" curve="-90"/>
<wire x1="27.94" y1="-1.285825" x2="25.384175" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="-1.27" x2="7.62" y2="1.27" width="0" layer="20" curve="-90"/>
<wire x1="7.62" y1="1.27" x2="25.384175" y2="1.27" width="0" layer="20"/>
<wire x1="33.02" y1="19.030875" x2="30.460875" y2="21.59" width="0" layer="20" curve="90"/>
<wire x1="30.460875" y1="21.59" x2="27.94" y2="19.069125" width="0" layer="20" curve="90"/>
<wire x1="27.94" y1="19.069125" x2="25.380875" y2="16.51" width="0" layer="20" curve="-90"/>
<wire x1="25.380875" y1="16.51" x2="7.59446875" y2="16.51" width="0" layer="20"/>
<wire x1="7.59446875" y1="16.51" x2="5.08" y2="19.02446875" width="0" layer="20" curve="-90"/>
<wire x1="5.08" y1="19.02446875" x2="2.51446875" y2="21.59" width="0" layer="20" curve="90"/>
<wire x1="2.51446875" y1="21.59" x2="0" y2="19.07553125" width="0" layer="20" curve="90"/>
<wire x1="0" y1="19.07553125" x2="0" y2="-1.27" width="0" layer="20"/>
<wire x1="0" y1="-1.27" x2="2.54" y2="-3.81" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="-3.81" x2="5.08" y2="-1.27" width="0" layer="20" curve="90"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>Matthew Reed 2013</text>
<text>RJ45 Breakout v1.1</text>
<hole x="2.54" y="19.05" drill="2.8"/>
<hole x="30.48" y="19.05" drill="2.8"/>
<hole x="2.54" y="-1.27" drill="2.8"/>
<hole x="30.48" y="-1.27" drill="2.8"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
<package name="SCREWTERMINAL-3.5MM-4_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4_LOCK" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4_LOCK" value=""/>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="GREEN"/>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="130"/>
</elements>
<signals>
<signal name="PIN8">
<contactref element="U$1" pad="8"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="PIN7">
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PIN6">
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PIN5">
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PIN4">
<contactref element="U$1" pad="4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="PIN3">
<contactref element="U$1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="PIN2">
<contactref element="U$1" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PIN1">
<contactref element="U$1" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
