<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="33.274" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="0" x2="8.89" y2="0" width="0" layer="20"/>
<wire x1="8.89" y1="0" x2="12.7" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="3.81" x2="12.7" y2="33.274" width="0" layer="20"/>
<wire x1="12.7" y1="33.274" x2="8.89" y2="37.084" width="0" layer="20" curve="90"/>
<wire x1="8.89" y1="37.084" x2="3.81" y2="37.084" width="0" layer="20"/>
<wire x1="3.81" y1="37.084" x2="0" y2="33.274" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SeniorDesign">
<packages>
<package name="SOIC8">
</package>
<package name="MAX44009">
</package>
<package name="SMALL_CU">
</package>
<package name="CU">
</package>
<package name="SENSORS-LOGO-SILK">
</package>
</packages>
</library>
<library name="SLAT-CON-JST-ZH">
<packages>
<package name="ZH-H-4-1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SeniorDesign" package="SOIC8" value="HIH6131-021-001"/>
<element name="U$2" library="SeniorDesign" package="MAX44009" value="MAX44009">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="0603-CAP" value="0.22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="SeniorDesign" package="SMALL_CU" value="SMALL_CU"/>
<element name="U$5" library="SeniorDesign" package="CU" value=""/>
<element name="U$6" library="SeniorDesign" package="SENSORS-LOGO-SILK" value=""/>
<element name="J1" library="SLAT-CON-JST-ZH" package="ZH-H-4-1" value="ZH-H-4-1"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="U$2" pad="P$7"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="6"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
