<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="34.29" x2="0" y2="5.08" width="0" layer="20"/>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="0" x2="43.0084" y2="0.04480625" width="0" layer="20"/>
<wire x1="43.0084" y1="0.04480625" x2="48.0824" y2="5.124803125" width="0" layer="20" curve="89.943276"/>
<wire x1="48.0824" y1="5.124803125" x2="48.0824" y2="34.33479375" width="0" layer="20"/>
<wire x1="48.0824" y1="34.33479375" x2="42.9964" y2="39.414790625" width="0" layer="20" curve="90.067672"/>
<wire x1="42.9964" y1="39.414790625" x2="5.08" y2="39.37" width="0" layer="20"/>
<wire x1="5.08" y1="39.37" x2="0" y2="34.29" width="0" layer="20" curve="90"/>
<text>+</text>
<text>-</text>
<text>HIGH VOLTAGE</text>
<text>HIGH VOLTAGE</text>
<text>HIGH VOLTAGE</text>
<hole x="31.496" y="22.86" drill="2.54"/>
<hole x="31.496" y="22.225" drill="2.54"/>
<hole x="31.496" y="21.59" drill="2.54"/>
<hole x="31.496" y="20.955" drill="2.54"/>
<hole x="31.496" y="20.32" drill="2.54"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10_LOCK">
</package>
<package name="GEIGER_TUBE">
</package>
<package name="SOT23-3">
</package>
<package name="SOD-323">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="1206">
</package>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="TRIMPOT-3MM">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="SeniorDesign">
<packages>
<package name="B82801B724A60">
</package>
<package name="SMALL_CU">
</package>
<package name="KANNING-PLACE">
</package>
<package name="KROENING-PLACE">
</package>
<package name="RIPPERGER-PLACE">
</package>
<package name="ZONCA-PLACE">
</package>
<package name="GEIGER-LOGO-SILK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="PS12">
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X10_LOCK" value="M10LOCK"/>
<element name="JP2" library="SparkFun" package="1X10_LOCK" value="M10LOCK"/>
<element name="U$1" library="SparkFun" package="GEIGER_TUBE" value="GEIGER_TUBELND712"/>
<element name="Q1" library="SparkFun" package="SOT23-3" value="MOSFET-NCHANNELSMD"/>
<element name="D1" library="SparkFun" package="SOD-323" value=""/>
<element name="D2" library="SparkFun" package="SOD-323" value=""/>
<element name="D3" library="SparkFun" package="SMA-DIODE" value=""/>
<element name="C1" library="SparkFun" package="1206" value=".022uF"/>
<element name="R1" library="SparkFun" package="0603-RES" value="1M"/>
<element name="R2" library="SparkFun" package="0603-RES" value="10M"/>
<element name="C2" library="SparkFun" package="0603-CAP" value="47pF"/>
<element name="C3" library="SparkFun" package="0603-CAP" value="100uF"/>
<element name="C4" library="SparkFun" package="0603-CAP" value=""/>
<element name="SNUB" library="SparkFun" package="SMA-DIODE" value=""/>
<element name="R3" library="SparkFun" package="0603-RES" value=""/>
<element name="R4" library="SparkFun" package="TRIMPOT-3MM" value="10k"/>
<element name="C5" library="SparkFun" package="0603-CAP" value="1nF"/>
<element name="R5" library="SparkFun" package="0603-RES" value="1K"/>
<element name="R6" library="SparkFun" package="0603-RES" value="1.8K"/>
<element name="Q2" library="SparkFun" package="SOT23" value=""/>
<element name="C6" library="SparkFun" package="0603-CAP" value="4.7uF"/>
<element name="U$2" library="SeniorDesign" package="B82801B724A60" value="TRANSFORMERX"/>
<element name="IC2" library="74xx-eu" package="SO14" value="74HC14D"/>
<element name="C7" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="C8" library="SparkFun" package="0603-CAP" value="1nF"/>
<element name="SP3" library="adafruit" package="PS12" value="SPEAKER/PS12"/>
<element name="R7" library="SparkFun" package="0603-RES" value=""/>
<element name="LED1" library="SparkFun" package="LED-0603" value=""/>
<element name="IC1" library="microchip" package="SOT23-5L" value="24LC00OT">
<attribute name="OC_NEWARK" value="62K0574"/>
<attribute name="MPN" value="24LC00T-I/OT"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="9757864"/>
</element>
<element name="IC3" library="linear" package="SO08" value="TLC3702"/>
<element name="R8" library="SparkFun" package="0603-RES" value="1K"/>
<element name="R9" library="SparkFun" package="0603-RES" value="9.1K"/>
<element name="R10" library="SparkFun" package="0603-RES" value="2M"/>
<element name="R11" library="SparkFun" package="0603-RES" value="10K"/>
<element name="Q3" library="SparkFun" package="SOT23-3" value="MOSFET-PCHANNELSMD"/>
<element name="U$3" library="SeniorDesign" package="SMALL_CU" value=""/>
<element name="U$6" library="SeniorDesign" package="KANNING-PLACE" value=""/>
<element name="U$7" library="SeniorDesign" package="KROENING-PLACE" value=""/>
<element name="U$8" library="SeniorDesign" package="RIPPERGER-PLACE" value=""/>
<element name="U$9" library="SeniorDesign" package="ZONCA-PLACE" value=""/>
<element name="U$5" library="SeniorDesign" package="GEIGER-LOGO-SILK" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="VBAT">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="3"/>
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="14"/>
<contactref element="C7" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="SP3" pad="P$2"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC3" pad="8"/>
<contactref element="Q3" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="6"/>
</signal>
<signal name="PD4">
<contactref element="JP1" pad="7"/>
</signal>
<signal name="PD5">
<contactref element="JP1" pad="8"/>
</signal>
<signal name="PD6">
<contactref element="JP1" pad="9"/>
</signal>
<signal name="PD7">
<contactref element="JP1" pad="10"/>
</signal>
<signal name="SCL">
<contactref element="JP2" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="PA0">
<contactref element="JP2" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="SP3" pad="P$1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="PA1">
<contactref element="JP2" pad="4"/>
</signal>
<signal name="PA2">
<contactref element="JP2" pad="5"/>
</signal>
<signal name="PA3">
<contactref element="JP2" pad="6"/>
</signal>
<signal name="PA4">
<contactref element="JP2" pad="7"/>
</signal>
<signal name="PA5">
<contactref element="JP2" pad="8"/>
</signal>
<signal name="PA6">
<contactref element="JP2" pad="9"/>
</signal>
<signal name="PA7">
<contactref element="JP2" pad="10"/>
</signal>
<signal name="HV">
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="VCC"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="SNUB" pad="C"/>
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="D2" pad="1"/>
<contactref element="R4" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="R4" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R4" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="PULSE">
<contactref element="Q1" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="C2" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="R5" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D3" pad="A"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$43">
<contactref element="SNUB" pad="A"/>
<contactref element="U$2" pad="8"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R7" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="U$2" pad="7"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="CUT">
<contactref element="Q3" pad="1"/>
<contactref element="IC3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
