<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<packages>
<package name="SOIC8">
</package>
<package name="SOT23-5">
</package>
<package name="SOIC8HEAT">
</package>
</packages>
<symbols>
<symbol name="PCF8523">
<description>The PCF8523 is a CMOS1 Real-Time Clock (RTC) and calendar optimized for low power
consumption.</description>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="OSCI"/>
<pin name="OSCO"/>
<pin name="VBAT"/>
<pin name="\INT1/CLKOUT"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="MCP9800">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="ALERT"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="IFX91041EJ">
<pin name="SYNC"/>
<pin name="VS"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="BDS"/>
<pin name="BUO"/>
<pin name="FB"/>
<pin name="COMP"/>
</symbol>
<symbol name="TPS76833QD">
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="!EN"/>
<pin name="GND"/>
<pin name="PG"/>
<pin name="NC"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PCF8523">
<gates>
<gate name="G$1" symbol="PCF8523"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="\INT1/CLKOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP9800">
<gates>
<gate name="G$1" symbol="MCP9800"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ALERT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IFX91041EJ">
<gates>
<gate name="G$1" symbol="IFX91041EJ"/>
</gates>
<devices>
<device name="" package="SOIC8HEAT">
<connects>
<connect gate="G$1" pin="BDS" pad="5"/>
<connect gate="G$1" pin="BUO" pad="6"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="EN" pad="7"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="2 9"/>
<connect gate="G$1" pin="SYNC" pad="1"/>
<connect gate="G$1" pin="VS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS76833QD">
<gates>
<gate name="G$1" symbol="TPS76833QD"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="4"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="PG" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
